;*******************************************************************************
;*                                                                            **
;*                     I N T E L   P R O P R I E T A R Y                      **
;*                                                                            **
;*   COPYRIGHT (c) 1993-2004 BY INTEL CORPORATION. ALL RIGHTS RESERVED.  NO   **
;*   PART  OF  THIS  PROGRAM OR PUBLICATION MAY BE REPRODUCED, TRANSMITTED,   **
;*   TRANSCRIBED, STORED IN A RETRIEVAL  SYSTEM,  OR  TRANSLATED  INTO  ANY   **
;*   LANGUAGE OR COMPUTER LANGUAGE IN ANY FORM OR BY ANY MEANS, ELECTRONIC,   **
;*   MECHANICAL, MAGNETIC, OPTICAL, CHEMICAL, MANUAL, OR OTHERWISE, WITHOUT   **
;*   THE PRIOR WRITTEN PERMISSION OF :                                        **
;*                                                                            **
;*                             INTEL CORPORATION                              **
;*                                                                            **
;*                          2200 MISSION COLLEGE BLVD                         **
;*                                                                            **
;*                     SANTA CLARA, CALIFORNIA 95052-8119                     **
;*                                                                            **
;*******************************************************************************
;
;*******************************************************************************
; NET5579x.INF
; $Revision: 35 $
;
; Intel 8255x-based PCI Ethernet Adapters
; PnP install script for Windows 9x
;   Version 7.1.12.0

[Version]
Signature       = "$Chicago$"
Class           = Net
ClassGUID       = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider        = %V_INTEL%
;CatalogFile     = e100b9x.cat
DriverVer       = 02/10/2004,7.1.12.0

[Manufacturer]
%V_INTEL%   = Intel

[ControlFlags]
ExcludeFromSelect =  \
                        PCI\VEN_8086&DEV_1229&SUBSYS_00018086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00028086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00038086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00048086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00058086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00068086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00078086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00088086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_000B8086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_000C8086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00118086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00138086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00308086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00418086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10098086&REV_05,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10138086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10308086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10418086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10518086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10528086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10F08086&REV_04,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10F08086&REV_05,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_21038086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_21048086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_21058086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_21068086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_21088086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_22018086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_22048086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_22058086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_22068086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_22078086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_22088086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_24028086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_24078086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_24088086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_24098086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_240F8086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_24108086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_24118086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_24128086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_24138086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_30078086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_005C1014&REV_04,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_005C1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_105C1014&REV_08,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_105C1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_01F11014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_01F21014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_01BC1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_02071014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_023F1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_305C1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_405C1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_505C1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_605C1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_705C1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_805C1014,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10C0103C,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10C3103C,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10CA103C,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10CB103C,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10E3103C,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_10E4103C,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_1200103C,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_30010E11,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_30020E11,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_30030E11,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_30040E11,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_30050E11,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_30060E11,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_30070E11,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_30118086,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_009B1028&REV_08,\
                        PCI\VEN_8086&DEV_1229&SUBSYS_00708086,\
                        PCI\VEN_8086&DEV_1229&REV_01,\
                        PCI\VEN_8086&DEV_1229&REV_02,\
                        PCI\VEN_8086&DEV_1229&REV_04,\
                        PCI\VEN_8086&DEV_1229&REV_05,\
                        PCI\VEN_8086&DEV_1229&REV_08,\
                        PCI\VEN_8086&DEV_1229&REV_09,\
                        PCI\VEN_8086&DEV_1229&REV_0C,\
                        PCI\VEN_8086&DEV_1229&REV_0D,\
                        PCI\VEN_8086&DEV_1229&REV_0E,\
                        PCI\VEN_8086&DEV_1229&REV_0F,\
                        PCI\VEN_8086&DEV_1229&REV_10,\
                        PCI\VEN_8086&DEV_1059


[Intel]
; DisplayName                Section        DeviceID
; -----------                -------        --------
%PCIE10PPCI.DeviceDesc%  =E10P.ndi,PCI\VEN_8086&DEV_1229&SUBSYS_00038086

%PCIE100BTX.DeviceDesc%         = E100B.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_00018086
%PCIE100BT4.DeviceDesc%         = E100B.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_00028086
%PCIE100RWU.DeviceDesc%         = E100B.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_00048086
%I557IFE.DeviceDesc%            = E100B.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_00058086
%I557IFEWFM.DeviceDesc%         = E100B.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_00068086

%I558IFE.DeviceDesc%            = D101.ndi,     PCI\VEN_8086&DEV_1229&SUBSYS_00078086
%I558IFEWFM.DeviceDesc%         = D101.ndi,     PCI\VEN_8086&DEV_1229&SUBSYS_00088086
%PCIE100PLUS.DeviceDesc%        = D101r5.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_00098086
%PCIE100MAN.DeviceDesc%         = D101r5.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_000A8086

%PCIE100PLUS.DeviceDesc%        = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_000B8086
%PCIE100MAN.DeviceDesc%         = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_000C8086
%PCIE100AOL.DeviceDesc%         = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_000D8086
%PCIE100MANAOL.DeviceDesc%      = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_000E8086
%PCIE100S0.DeviceDesc%          = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_000F8086

%PCIE100S.DeviceDesc%           = D101S.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_00108086
%PCIE100S.DeviceDesc%           = D101S.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_00118086
%PCIE100SADV.DeviceDesc%        = D101S.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_00128086
%PCIE100SADV.DeviceDesc%        = D101S.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_00138086

%PCIE100MANAOLGC.DeviceDesc%    = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_00308086
%PCIE100S0.DeviceDesc%          = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_00318086
%PCIE100Sx.DeviceDesc%          = D102SC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_00408086
%PCIE100Sx.DeviceDesc%          = D102SC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_00418086
%PCIE100S0.DeviceDesc%          = D102SCN.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_00428086

%PCIE100Sx.DeviceDesc%          = D102mC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_00508086
%PCIE100Sx.DeviceDesc%          = D102mC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_00518086
%PCIE100DUALx.DeviceDesc%       = D102m0.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10148086
%PCIE100DUALSx.DeviceDesc%      = D102mS.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10158086
%PCIE100DUALSx.DeviceDesc%      = D102mS.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10168086
%PCIE100SxSVR.DeviceDesc%       = D102mS.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10508086

%PCIE100BSPLUSD.DeviceDesc%     = D102mC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_00608086
%PCIE100LAVON.DeviceDesc%       = Lavon.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_00708086
%PCIE100LAVON.DeviceDesc%       = Lavon.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_00718086

%PCIE100SxL.DeviceDesc%         = D102mC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_30108086
%PCIE100SxL.DeviceDesc%         = D102mC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_30118086



%PCIE100SERVER.DeviceDesc%      = D101.ndi,     PCI\VEN_8086&DEV_1229&SUBSYS_10098086&REV_04
%PCIE100SERVER.DeviceDesc%      = D101r5.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10098086&REV_05
%PCIE100SERVERW.DeviceDesc%     = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_100C8086
%PCIE100SSVR.DeviceDesc%        = D101SS.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10128086
%PCIE100SSVR.DeviceDesc%        = D101SS.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10138086
%PCIE100DUAL.DeviceDesc%        = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_10178086
%PCIE100MANAOLGS.DeviceDesc%    = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_10308086
%PCIE100SxSVR.DeviceDesc%       = D102SSC.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_10408086
%PCIE100SxSVR.DeviceDesc%       = D102SSC.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_10418086
%PCIE100S0SVR.DeviceDesc%       = D102SSCN.ndi, PCI\VEN_8086&DEV_1229&SUBSYS_10428086
%PCIE100S0SVR.DeviceDesc%       = D102SSCN.ndi, PCI\VEN_8086&DEV_1229&SUBSYS_10518086
%PCIE100S0SVR.DeviceDesc%       = D102SSCN.ndi, PCI\VEN_8086&DEV_1229&SUBSYS_10528086
%PCIE100DUAL.DeviceDesc%        = D101.ndi,     PCI\VEN_8086&DEV_1229&SUBSYS_10F08086&REV_04
%PCIE100DUAL.DeviceDesc%        = D101r5D.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10F08086&REV_05
%PCIE100BSPLUSS.DeviceDesc%     = D102mS.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10608086

%I559IFE.DeviceDesc%            = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_30008086
%I559IFEAOL.DeviceDesc%         = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_30018086
%I559IFEAOLII.DeviceDesc%       = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_30028086
%PCIE100SxL.DeviceDesc%         = D102SC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_30068086
%PCIE100SxL.DeviceDesc%         = D102SC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_30078086
%PCIE100S0L.DeviceDesc%         = D102SCN.ndi,  PCI\VEN_8086&DEV_1229&SUBSYS_30088086

; IBM with intel device name

%I559CLONPCI.DeviceDesc%        = D101S.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_B2090E11
%I559IFEAOLCPQ.DeviceDesc%      = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_30010E11
%I559IFEAOLCPQ.DeviceDesc%      = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_30020E11
%I559IFEAOLCPQ.DeviceDesc%      = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_30030E11
%I559IFEAOLCPQ.DeviceDesc%      = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_30040E11
%I559IFEAOLCPQ.DeviceDesc%      = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_30050E11
%I559IFEAOLCPQ.DeviceDesc%      = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_30060E11
%I559IFEAOLCPQ.DeviceDesc%      = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_30070E11

%HPTX.DeviceDesc%               = E100B.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_10C0103C
%HPTX.DeviceDesc%               = D101r5.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10C3103C
%HPTX.DeviceDesc%               = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_10CA103C
%HPTX.DeviceDesc%               = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_10CB103C
%HPTX.DeviceDesc%               = D102SC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10E3103C
%HPTX.DeviceDesc%               = D102SC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_10E4103C
%HPTX.DeviceDesc%               = E100B.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_1200103C
%HPTX.DeviceDesc%               = D102m0.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_1273103C

%IBMFE9.DeviceDesc%             = D101M.ndi,    PCI\VEN_8086&DEV_1229&SUBSYS_01BC1014
%IBMFED.DeviceDesc%             = D102SC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_02071014
%IBMFED.DeviceDesc%             = D102SC.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_023F1014

;Dell Viper
%PCIE100B.DeviceDesc%           = D101MG.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_009B1028&REV_08
%PCIE100B.DeviceDesc%           = D101MG.ndi,   PCI\VEN_8086&DEV_1229&SUBSYS_01061028&REV_08

;Intel Generic catchalls
%PCIE100B.DeviceDesc%           = E100B.ndi,    PCI\VEN_8086&DEV_1229&REV_01
%PCIE100B.DeviceDesc%           = E100B.ndi,    PCI\VEN_8086&DEV_1229&REV_02
%PCIE100B.DeviceDesc%           = D101.ndi,     PCI\VEN_8086&DEV_1229&REV_04
%PCIE100B.DeviceDesc%           = D101r5.ndi,   PCI\VEN_8086&DEV_1229&REV_05
%PCIE100B.DeviceDesc%           = D101MG.ndi,   PCI\VEN_8086&DEV_1229&REV_08
%PCIE100B.DeviceDesc%           = D101SG.ndi,   PCI\VEN_8086&DEV_1229&REV_09
%PCIE100B.DeviceDesc%           = D102SCNG.ndi, PCI\VEN_8086&DEV_1229&REV_0C
%PCIE100B.DeviceDesc%           = D102mG.ndi,   PCI\VEN_8086&DEV_1229&REV_0D
%PCIE100B.DeviceDesc%           = D102mG.ndi,   PCI\VEN_8086&DEV_1229&REV_0E
%PCIE100LAVONLOM.DeviceDesc%    = Lavon.ndi,    PCI\VEN_8086&DEV_1229&REV_0F
%PCIE100LAVONLOM.DeviceDesc%    = Lavon.ndi,    PCI\VEN_8086&DEV_1229&REV_10
%PCIE100LAVONMB.DeviceDesc%     = Lavonmb.ndi,  PCI\VEN_8086&DEV_1059&REV_0F
%PCIE100LAVONMB.DeviceDesc%     = Lavonmb.ndi,  PCI\VEN_8086&DEV_1059&REV_10

;--- 82557 Rev 1, 2
;
[E100B.ndi]
DriverVer       = 03/04/2003,7.0.26.0
DelReg          = 8255x_Legacy.DelReg, SpeedDpx.DelReg
AddReg          = Speed100.reg, 82557.reg, e100b.ndi.reg, PowerSave.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82558 Rev 4
;
[D101.ndi]
DriverVer       = 03/04/2003,7.0.26.0
DelReg          = 8255x_Legacy.DelReg, SpeedDpx.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, e100b.ndi.reg, PowerSave.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82558 Rev 5
;
[D101r5.ndi]
DriverVer       = 03/04/2003,7.0.26.0
DelReg          = 8255x_Legacy.DelReg, SpeedDpx.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, PowerSave.reg, e100b.ndi.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82558 Rev 5 (Dual)
;
[D101r5D.ndi]
DriverVer       = 03/04/2003,7.0.26.0
DelReg          = 8255x_Legacy.DelReg, SpeedDpx.DelReg, 82558BDelReg.DelReg, 82558r5dDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, e100b.ndi.reg, LogLinkState.reg, WakeOnDisable.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82559 Rev 8
;
[D101M.ndi]
DriverVer       = 03/04/2003,7.0.26.0
DelReg          = SpeedDpx.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, e100b.ndi.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82559 Rev 8 Generic
;
[D101MG.ndi]
DriverVer       = 03/04/2003,7.0.26.0
DelReg          = SpeedDpx.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, EnableLLPD.reg, LLPDD_OFF.reg, e100b.ndi.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82559 Rev 9 Security
;
[D101S.ndi]
DriverVer       = 03/04/2003,7.0.26.0
DelReg          = SpeedDpx.DelReg, TaskOffload.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, e100b.ndi.reg, Security.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82559 Rev 9 Security Generic
;
[D101SG.ndi]
DriverVer       = 03/04/2003,7.0.26.0
DelReg          = SpeedDpx.DelReg, TaskOffload.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, EnableLLPD.reg, LLPDD_OFF.reg, e100b.ndi.reg, Security.reg, SecOff.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- D101S Rev 9 Server
;
[D101SS.ndi]
DriverVer       = 03/04/2003,7.0.26.0
DelReg          = SpeedDpx.DelReg, TaskOffload.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, e100b.ndi.reg, Security.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev C Server
;
[D102SC.ndi]
DriverVer       = 03/04/2003,7.0.26.0
DelReg          = TaskOffload.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, e100b.ndi.reg, Security.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev C
;
[D102SCN.ndi]
DriverVer       = 03/04/2003,7.0.26.0
DelReg          = TaskOffload.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, e100b.ndi.reg, SecDisable.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev C Generic
;
[D102SCNG.ndi]
DriverVer       = 03/04/2003,7.0.26.0
DelReg          = TaskOffload.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, EnableLLPD.reg, LLPDD_OFF.reg, e100b.ndi.reg, Security.reg, SecOff.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev C Security Server
;
[D102SSC.ndi]
DriverVer       = 03/04/2003,7.0.26.0
DelReg          = TaskOffload.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, e100b.ndi.reg, Security.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev C Server
;
[D102SSCN.ndi]
DriverVer       = 03/04/2003,7.0.26.0
DelReg          = TaskOffload.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, e100b.ndi.reg, SecDisable.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev C MiniPCI Security
;
[D102MPS.ndi]
DriverVer       = 03/04/2003,7.0.26.0
DelReg          = TaskOffload.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, EnableLLPD.reg, e100b.ndi.reg, Security.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev D Server
;
[D102mS.ndi]
DriverVer       = 03/04/2003,7.0.26.0
DelReg          = TaskOffload.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, e100b.ndi.reg, Security.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev D Client
;
[D102mC.ndi]
DriverVer       = 03/04/2003,7.0.26.0
DelReg          = TaskOffload.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, e100b.ndi.reg, Security.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev D Client Mobile
;
[D102mCm.ndi]
DriverVer       = 03/04/2003,7.0.26.0
DelReg          = TaskOffload.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, e100b.ndi.reg, Security.reg, EnableLLPD.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev D Server NoDes
;
[D102m0.ndi]
DriverVer       = 03/04/2003,7.0.26.0
DelReg          = 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, PowerSave.reg, e100b.ndi.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev F Lavon mobile
;
[Lavonmb.ndi]
DriverVer       = 03/04/2003,7.0.26.0
DelReg          = 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnableLLPD.reg, PowerSave.reg, EnablePME.reg, e100b.ndi.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev D Generic
;
[D102mG.ndi]
DriverVer       = 03/04/2003,7.0.26.0
DelReg          = TaskOffload.DelReg, 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnableLLPD.reg, PowerSave.reg, EnablePME.reg, e100b.ndi.reg, Security.reg, SecOff.reg, LLPDD_OFF.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- 82550 Rev F Lavon
;
[Lavon.ndi]
DriverVer       = 03/04/2003,7.0.26.0
DelReg          = 82558BDelReg.DelReg
AddReg          = Speed100.reg, 82557.reg, AcpiWol.reg, 82558.reg, 82558B.reg, EnablePME.reg, e100b.ndi.reg, PowerSave.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- Intel(R) PRO/10+ PCI Adapter
;
[E10P.ndi]
DriverVer       = 03/04/2003,7.0.26.0
DelReg          = 8255x_Legacy.DelReg, SpeedDpx.DelReg
AddReg          = Speed10.reg, 82557.reg, e100b.ndi.reg, PowerSave.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- Common 82557 NDI parameters
;
[82557.reg]
HKR,Ndi\Params\NumRfd,                ParamDesc,  0, "Receive Buffers"
HKR,Ndi\Params\NumRfd,                Type,       0, "int"
HKR,Ndi\Params\NumRfd,                Default,    0, "48"
HKR,Ndi\Params\NumRfd,                Min,        0, "8"
HKR,Ndi\Params\NumRfd,                Max,        0, "1024"
HKR,Ndi\Params\NumRfd,                Step,       0, "1"
HKR,Ndi\Params\NumRfd,                Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\NumRfd,   MiniHelp,   0, "Number of buffers used by the driver when copying data to the protocol memory."

HKR,Ndi\Params\NumTcb,                ParamDesc,  0, "Transmit Control Blocks"
HKR,Ndi\Params\NumTcb,                Type,       0, "int"
HKR,Ndi\Params\NumTcb,                Default,    0, "16"
HKR,Ndi\Params\NumTcb,                Min,        0, "8"
HKR,Ndi\Params\NumTcb,                Max,        0, "64"
HKR,Ndi\Params\NumTcb,                Step,       0, "1"
HKR,Ndi\Params\NumTcb,                Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\NumTcb,   MiniHelp,   0, "Sets the number of control blocks available for adapter use."

HKR,Ndi\Params\NumCoalesce,           ParamDesc,  0, "Coalesce Buffers"
HKR,Ndi\Params\NumCoalesce,           Type,       0, "int"
HKR,Ndi\Params\NumCoalesce,           Default,    0, "8"
HKR,Ndi\Params\NumCoalesce,           Min,        0, "1"
HKR,Ndi\Params\NumCoalesce,           Max,        0, "32"
HKR,Ndi\Params\NumCoalesce,           Step,       0, "1"
HKR,Ndi\Params\NumCoalesce,           Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\NumCoalesce, MiniHelp, 0, "Number of buffers available for transmits acceleration."

HKR,Ndi\Params\Adaptive_IFS,          ParamDesc,  0, "Adaptive Inter-Frame Spacing"
HKR,Ndi\Params\Adaptive_IFS,          Type,       0, "int"
HKR,Ndi\Params\Adaptive_IFS,          Default,    0, "1"
HKR,Ndi\Params\Adaptive_IFS,          Min,        0, "0"
HKR,Ndi\Params\Adaptive_IFS,          Max,        0, "255"
HKR,Ndi\Params\Adaptive_IFS,          Step,       0, "1"
HKR,Ndi\Params\Adaptive_IFS,          Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\Adaptive_IFS, MiniHelp, 0, "Compensates for excessive Ethernet packet collisions."

HKR,Ndi\Params\Threshold,             ParamDesc,  0, "Adaptive Transmit Threshold"
HKR,Ndi\Params\Threshold,             Type,       0, "int"
HKR,Ndi\Params\Threshold,             Default,    0, "200"
HKR,Ndi\Params\Threshold,             Min,        0, "0"
HKR,Ndi\Params\Threshold,             Max,        0, "200"
HKR,Ndi\Params\Threshold,             Step,       0, "1"
HKR,Ndi\Params\Threshold,             Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\Threshold, MiniHelp,  0, "Sets number of bytes before adapter empties its FIFO buffer. Actual value is 8 times setting."

HKR,Ndi\Params\HPQPriorityLevel,             ParamDesc,  0, "Priority Level Definition"
HKR,Ndi\Params\HPQPriorityLevel,             Type,       0, "int"
HKR,Ndi\Params\HPQPriorityLevel,             Default,    0, "4"
HKR,Ndi\Params\HPQPriorityLevel,             Min,        0, "0"
HKR,Ndi\Params\HPQPriorityLevel,             Max,        0, "7"
HKR,Ndi\Params\HPQPriorityLevel,             Step,       0, "1"
HKR,Ndi\Params\HPQPriorityLevel,             Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\HPQPriorityLevel, MiniHelp,  0, "Sets the controlled cutoff level for using HPQ."

HKR,Ndi\Params\UcodeSW,               ParamDesc,  0, "Adaptive Technology"
HKR,Ndi\Params\UcodeSW,               Type,       0, "enum"
HKR,Ndi\Params\UcodeSW,               Default,    0, "1"
HKR,Ndi\Params\UcodeSW\Enum,          "1",        0, "On"
HKR,Ndi\Params\UcodeSW\Enum,          "0",        0, "Off"
HKR,PROSetNdi\NdiExt\Params\UcodeSW,  MiniHelp,   0, "Enables/Disables the Adaptive Technology performance feature."

HKR,Ndi\Params\Coalesce,              ParamDesc,  0, "PCI Bus Efficiency"
HKR,Ndi\Params\Coalesce,              Type,       0, "enum"
HKR,Ndi\Params\Coalesce,              Default,    0, "0"
HKR,Ndi\Params\Coalesce\Enum,         "1",        0, %Enabled%
HKR,Ndi\Params\Coalesce\Enum,         "0",        0, %Disabled%
HKR,PROSetNdi\NdiExt\Params\Coalesce, MiniHelp,   0, "Coalesces transmit packets into single buffer before sending them to network."

HKR,Ndi\Params\AlwaysConnectGoal,              ParamDesc,  0, "Low Resource Connectivity"
HKR,Ndi\Params\AlwaysConnectGoal,              Type,       0, "enum"
HKR,Ndi\Params\AlwaysConnectGoal,              Default,    0, "1"
HKR,Ndi\Params\AlwaysConnectGoal\Enum,         "1",        0, %Enabled%
HKR,Ndi\Params\AlwaysConnectGoal\Enum,         "0",        0, %Disabled%
HKR,PROSetNdi\NdiExt\Params\AlwaysConnectGoal, MiniHelp,   0,  "Try to load the driver in low resources environment."

HKR,Ndi\Params\NetworkAddress,  ParamDesc,  0, "Locally Administered Address"
HKR,Ndi\Params\NetworkAddress,  Type,       0, "edit"
HKR,Ndi\Params\NetworkAddress,  Default,    0, "0"
HKR,NDI\params\NetworkAddress,  LimitText,  0, "12"
HKR,NDI\params\NetworkAddress,  UpperCase,  0, "1"
HKR,PROSetNdi\NdiExt\Params\NetworkAddress,  MiniHelp,   0, "By default, an address is not present and the value field is left blank. To set a LAA in Intel(R) PROSet, enter one in the value field. Note: To set a LAA in Device Manager, select the Value option and enter an address in the field provided."

HKR,Ndi\Params\ConfigIFS,                ParamDesc,  0, "Retransmit Inter-Frame Spacing"
HKR,Ndi\Params\ConfigIFS,                Type,       0, "int"
HKR,Ndi\Params\ConfigIFS,                Default,    0, "6"
HKR,Ndi\Params\ConfigIFS,                Min,        0, "0"
HKR,Ndi\Params\ConfigIFS,                Max,        0, "15"
HKR,Ndi\Params\ConfigIFS,                Step,       0, "1"
HKR,Ndi\Params\ConfigIFS,                Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\ConfigIFS,   MiniHelp,   0, "Compensates for excessive Ethernet packet collisions by controlling retransmit timing."

HKR,,PcNic,                     0, "1"
HKR,,MWIEnable,                 2, "0"
HKR,,AdaptiveStalledInterrupts, 2, "1"
HKR,,AdaptiveCarrierLoss,       2, "1"
HKR,,AdaptiveTransmitMethod,    2, "1"
HKR,,Threshold,                 0, "200"

HKR,,DeviceVxDsPrefix,          0, "e100b"

;--- 82558 ACPI Wake On LAN parameter
;
[AcpiWol.reg]
HKR,Ndi\Params\AcpiWol,               ParamDesc,  0, "ACPI Wake On LAN"
HKR,Ndi\Params\AcpiWol,               Type,       0, "enum"
HKR,Ndi\Params\AcpiWol,               Default,    0, "1"
HKR,Ndi\Params\AcpiWol\Enum,          "1",        0, %Enabled%
HKR,Ndi\Params\AcpiWol\Enum,          "0",        0, %Disabled%
HKR,PROSetNdi\NdiExt\Params\AcpiWol,  MiniHelp,   0, "Enables or disables the Magic Packet* service for Wake On LAN with Windows 98 version 4.10.1998."

HKLM,System\CurrentControlSet\Services\VxD\ACPIWOL,Start,     1, 00
HKLM,System\CurrentControlSet\Services\VxD\ACPIWOL,StaticVxD, 0, "WOL558.vxd"

;--- Log Link State Event
;
[LogLinkState.reg]
HKR,,LogLinkStateEvent, 0,      "1"

;--- 82558 specifics
;
[82558.reg]
; 802.1p/802.1q Packet Tagging
HKR,Ndi\Params\TaggingMode,         ParamDesc,  0, "QoS Packet Tagging"
HKR,Ndi\Params\TaggingMode,         Type,       0, "enum"
HKR,Ndi\Params\TaggingMode,         Default,    0, "0"
HKR,Ndi\Params\TaggingMode\Enum,    "1",        0, %Enabled%
HKR,Ndi\Params\TaggingMode\Enum,    "0",        0, %Disabled%
HKR,PROSetNdi\NdiExt\Params\TaggingMode, MiniHelp, 0, "Send and receive IEEE Tagged frames (802.3ac/802.1p/802.1Q)."

; Flow Control Settings
HKR,Ndi\Params\FlowControl,              ParamDesc,  0, "Flow Control Settings"
HKR,Ndi\Params\FlowControl,              Type,       0, "enum"
HKR,Ndi\Params\FlowControl,              Default,    0, "3"
HKR,Ndi\Params\FlowControl\Enum,         "3",        0, "Generate and Respond"
HKR,Ndi\Params\FlowControl\Enum,         "2",        0, "Respond"
HKR,Ndi\Params\FlowControl\Enum,         "1",        0, "Generate"
HKR,Ndi\Params\FlowControl\Enum,         "0",        0, "Off"
HKR,PROSetNdi\NdiExt\Params\FlowControl, MiniHelp,   0, "Pauses packet transmission on receipt of full flow control frame and Send full flow control frame to notify the other side to stop transmission."
HKR,,				   	FlowControl, 0, "3"

; Adaptive Performance Tuning
HKR,PROSetNdi\Params\CPUSaver,        ParamDesc,  0, "Adaptive Performance Tuning"
HKR,PROSetNdi\Params\CPUSaver,        Type,       0, "slider"
HKR,PROSetNdi\Params\CPUSaver,        Default,    0, "512"
HKR,,CPUSaver,                                    0, "512"
HKR,PROSetNdi\Params\CPUSaver,        LeftLabel,  0, "Adapter Bandwidth"
HKR,PROSetNdi\Params\CPUSaver,        RightLabel, 0, "CPU Utilization"
HKR,PROSetNdi\Params\CPUSaver,        MiniHelp,   0, "Sets optimal point of CPU/Adapter performance for this system."
HKR,PROSetNdi\Params\CPUSaver\Values, "0",        0, "0"
HKR,PROSetNdi\Params\CPUSaver\Values, "1",        0, "1"
HKR,PROSetNdi\Params\CPUSaver\Values, "2",        0, "512"
HKR,PROSetNdi\Params\CPUSaver\Values, "3",        0, "768"
HKR,PROSetNdi\Params\CPUSaver\Values, "4",        0, "1024"
HKR,PROSetNdi\Params\CPUSaver\Values, "5",        0, "1280"
HKR,PROSetNdi\Params\CPUSaver\Values, "6",        0, "1536"
HKR,PROSetNdi\Params\CPUSaver\Values, "7",        0, "1792"
HKR,PROSetNdi\Params\CPUSaver\Values, "8",        0, "2048"
HKR,PROSetNdi\Params\CPUSaver\Values, "9",        0, "2304"
HKR,PROSetNdi\Params\CPUSaver\Values, "10",       0, "2560"
HKR,PROSetNdi\Params\CPUSaver\Values, "11",       0, "2816"
HKR,PROSetNdi\Params\CPUSaver\Values, "12",       0, "3072"
HKR,PROSetNdi\Params\CPUSaver\Values, "13",       0, "3328"
HKR,PROSetNdi\Params\CPUSaver\Values, "14",       0, "3584"
HKR,PROSetNdi\Params\CPUSaver\Values, "15",       0, "3840"
HKR,PROSetNdi\Params\CPUSaver\Values, "16",       0, "4096"

;--- 82558 B Rev 5
;
[82558B.reg]
; WakeOn
HKR, Ndi\Params\WakeOn,       	  ParamDesc,          0, "Wake on Settings"
HKR, Ndi\Params\WakeOn,       	  default,            0, "246"
HKR, Ndi\Params\WakeOn\Enum,  	  "0",                0, %Disabled%
HKR, Ndi\Params\WakeOn\Enum,  	  "6",                0, "Wake on Magic Packet"
HKR, Ndi\Params\WakeOn\Enum,  	  "116",              0, "Wake on directed packet"
HKR, Ndi\Params\WakeOn\Enum,  	  "118",              0, "Wake on Magic & Directed"
HKR, Ndi\Params\WakeOn\Enum,      "246",              0, %OSControlled%
HKR, Ndi\Params\WakeOn,       	  type,               0, "enum"
HKR, Ndi\Params\WakeOn,       	  ExposeLevel,        0, "2"
HKR, Ndi\Params\WakeOn,       	  MiniHelp,           0, "Determines which packets can be enabled to Wake up the system (Direct Packets, Magic Packet etc.)."
HKR,,				  WakeOn, 	      0, "246"

;Wake on Link parameter
HKR, Ndi\Params\WakeOnLink,       ParamDesc,            0, %WakeOnLinkSettings%
HKR, Ndi\Params\WakeOnLink\Enum,  "0",                  0, %Disabled%
HKR, Ndi\Params\WakeOnLink\Enum,  "1",                  0, %OSControlled% 
HKR, Ndi\Params\WakeOnLink\Enum,  "2",                  0, %Forced%
HKR, Ndi\Params\WakeOnLink,       type,                 0, "enum"
;HKR, Ndi\Params\WakeOnLink,       ExposeLevel,        0, "2"
HKR, PROSetNdi\NdiExt\Params\WakeOnLink, MiniHelp,      0, %WakeOnLinkHelp% 

;--- Wake on disable - sets WakeOn registry key to 0
;
[WakeOnDisable.reg]
HKR,,				  WakeOn, 	      0, "0"

;--- 82559 Enable PME
;
[EnablePME.reg]
HKR,Ndi\Params\EnablePME,             ParamDesc,  0, "Enable PME"
HKR,Ndi\Params\EnablePME,             Type,       0, "enum"
HKR,Ndi\Params\EnablePME,             Default,    0, "2"
HKR,Ndi\Params\EnablePME\Enum,        "1",        0, %Enabled%
HKR,Ndi\Params\EnablePME\Enum,        "0",        0, %Disabled%
HKR,Ndi\Params\EnablePME\Enum,        "2",        0, "No Action"
HKR,Ndi\Params\EnablePME\Enum,        "255",      0, "Hardware Default"
HKR,PROSetNdi\NdiExt\Params\EnablePME, MiniHelp,  0, "Allows wake-up from APM power management when enabled. Disable shuts down LAN controller under ACPI"

;--- Clkrun
[Clkrun.reg]
HKR,,CLKRUN,                                      0, "1"

;--- Enable Power Down
;
[EnableLLPD.reg]
HKR,Ndi\Params\EnablePowerDownOnLinkLoss,      ParamDesc,  0, "Smart Power Down"
HKR,Ndi\Params\EnablePowerDownOnLinkLoss,      Type,       0, "enum"
HKR,Ndi\Params\EnablePowerDownOnLinkLoss,      Default,    0, "1"
HKR,Ndi\Params\EnablePowerDownOnLinkLoss\Enum, "1",        0, %Enabled%
HKR,Ndi\Params\EnablePowerDownOnLinkLoss\Enum, "0",        0, %Disabled%
HKR,PROSetNdi\NdiExt\Params\EnablePowerDownOnLinkLoss, MiniHelp, 0, "Removes adapter power when LAN cable disconnected."

HKR,Ndi\Params\LinkBasedLogin,              ParamDesc,  0, "Adaptive Link Response"
HKR,Ndi\Params\LinkBasedLogin,              Type,       0, "enum"
HKR,Ndi\Params\LinkBasedLogin,              Default,    0, "0"
HKR,Ndi\Params\LinkBasedLogin\Enum,         "1",        0, "On"
HKR,Ndi\Params\LinkBasedLogin\Enum,         "0",        0, "Off"
HKR,PROSetNdi\NdiExt\Params\LinkBasedLogin, MiniHelp,   0, "Enables Adaptive Link Response to check PHYLink status."

;--- Expose Power Mangement feature in Lavon
[PowerSave.reg]
HKR,,AutoPowerSaveModeEnabled, 0, "1"
HKR,,Force10MbOnD3, 0, "1"
HKR,,SavePowerNowEnabled,    0, "1"

[LLPDD_OFF.reg]
HKR,Ndi\Params\EnablePowerDownOnLinkLoss,      Default,    0, "0"

;--- Security
;
[Security.reg]
HKR,Ndi\Params\MaxNumSecAssoc,  ParamDesc,  0, %SecurityAssociations%
HKR,Ndi\Params\MaxNumSecAssoc,  Type,       0, "int"
HKR,Ndi\Params\MaxNumSecAssoc,  Default,    0, "64"     ; Client
HKR,Ndi\Params\MaxNumSecAssoc,  Min,        0, "1"
HKR,Ndi\Params\MaxNumSecAssoc,  Max,        0, "5000"
HKR,Ndi\Params\MaxNumSecAssoc,  Step,       0, "1"
HKR,Ndi\Params\MaxNumSecAssoc,  Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\MaxNumSecAssoc, MiniHelp, 0, "Simultaneous Security Associations that can be offloaded to the adapters co-processor."

HKR,Ndi\Params\IPSecEnabled,     ParamDesc,  0, %IPSecEnabled%
HKR,Ndi\Params\IPSecEnabled,     Type,       0, "enum"
HKR,Ndi\Params\IPSecEnabled,     Default,    0, "1"
HKR,Ndi\Params\IPSecEnabled\Enum,"0",        0, %Off%
HKR,Ndi\Params\IPSecEnabled\Enum,"1",        0, %On%
HKR,PROSetNdi\NdiExt\Params\IPSecEnabled, MiniHelp, 0, "Saves CPU cycles if set to correspond to the adapter type. Range: Enabled | Disabled"

HKR,,IPSecTunnelMode, 2, "1"
HKR,,MaxNumSecAssoc,  2, "64"

[SecSerDef.reg]
HKR,Ndi\Params\MaxNumSecAssoc,  Default,    0, "1000"   ; Server

[SecOff.reg]
HKR,Ndi\Params\IPSecEnabled,     Default,    0, "0"

[SecDisable.reg]
HKR,,IPSecEnabled,    0, "0"

;--- CPUSaver override for Cardbus
;
[CPUSaverOverride.reg]
HKR,PROSetNdi\Params\CPUSaver,  Default,    0, "1"
HKR,,CPUSaver,                              0, "1"

;--- Speed Duplex Mode common base 10Mb
;
[Speed10.reg]
HKR, Ndi\params\SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR, Ndi\params\SpeedDuplex,       default,    0, "1"
HKR, Ndi\params\SpeedDuplex,       type,       0, "enum"
HKR, Ndi\params\SpeedDuplex\enum,  "1",        0, %10Mb-Half-Duplex%
HKR, Ndi\params\SpeedDuplex\enum,  "2",        0, %10Mb-Full-Duplex%
HKR, PROSetNdi\NdiExt\params\SpeedDuplex, MiniHelp,    0, "Sets link speed to 10 Mbps and duplex to half or full. Must coincide with switch port or no link will occur."
HKR, PROSetNdi\NdiExt\params\SpeedDuplex, ExposeLevel, 0, "2"

;--- Speed Duplex Mode common base 10/100Mb
;
[Speed100.reg]
HKR, Ndi\params\SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR, Ndi\params\SpeedDuplex,       default,    0, "0"
HKR, Ndi\params\SpeedDuplex,       type,       0, "enum"
HKR, Ndi\params\SpeedDuplex\enum,  "0",        0, %AutoDetect%
HKR, Ndi\params\SpeedDuplex\enum,  "1",        0, %10Mb-Half-Duplex%
HKR, Ndi\params\SpeedDuplex\enum,  "2",        0, %10Mb-Full-Duplex%
HKR, Ndi\params\SpeedDuplex\enum,  "3",        0, %100Mb-Half-Duplex%
HKR, Ndi\params\SpeedDuplex\enum,  "4",        0, %100Mb-Full-Duplex%
HKR, PROSetNdi\NdiExt\params\SpeedDuplex, MiniHelp,    0, "Sets link speed to 10/100 Mbps and duplex to half or full. Must coincide with switch port or no link will occur."
HKR, PROSetNdi\NdiExt\params\SpeedDuplex, ExposeLevel, 0, "2"

;--- Settings to be cleaned up
;
[8255x_Legacy.DelReg]
HKR,Ndi\Params\Eid
HKR,Ndi\Params\MapRegisters
HKR,,Eid
HKR,,MapRegisters

;Remove old TaskOffload registry keys
[TaskOffload.DelReg]
HKR,Ndi\Params\TaskOffload
HKR,,TaskOffload

[82558BDelReg.DelReg]
HKR, PROSetNdi\Params\WakeOn
HKR, Ndi\Params\WakeOn
HKR, Ndi\Params\WakeOnLink

[82558r5dDelReg.DelReg]
HKR,,AutoPowerSaveModeEnabled
HKR,,Force10MbOnD3


;--- Win9x NDI object registration
;
[E100B.ndi.reg]
HKR,,               DevLoader,        0, "*ndis"
HKR,,               DeviceVxDs,       0, "e100bnt5.sys"
HKR,,               EnumPropPages,    0, "netdi.dll,EnumPropPages"
HKR,,               Driver,           0, "e100bnt.sys"
HKR,NDIS,           LogDriverName,    0, "E100B"
HKR,NDIS,           MajorNdisVersion, 1, 03
HKR,NDIS,           MinorNdisVersion, 1, 0A
HKR,Ndi,            NdiInstaller,     0, "8255indi.dll,i557NdiProc"
HKR,Ndi,            DeviceID,         0, "PCI\VEN_8086&DEV_1229"
HKR,Ndi\Interfaces, DefUpper,         0, "ndis3"
HKR,Ndi\Interfaces, DefLower,         0, "ethernet"
HKR,Ndi\Interfaces, UpperRange,       0, "ndis3"
HKR,Ndi\Interfaces, LowerRange,       0, "ethernet"

;--- Uninstallation
;adapters not hardcoded to remove
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1059, 0, "82551"

HKLM,Software\Microsoft\Windows\CurrentVersion\Uninstall\PROSet,DisplayName, 0, "Intel(R) PRO Network Adapters and Drivers"
HKLM,Software\Microsoft\Windows\CurrentVersion\Uninstall\PROSet,UninstallString, 0, "8255xDel.exe"
HKLM,Software\Intel\Prounstl\Dins, e100b9x.din, 0, "8255x.Uninstall"

;--- Driver Install
;
; NDIS5
[E100B.ndis5]
CopyFiles = E100B.ndis5.CopyFiles

; NDIS4
[E100B.ndis4]
CopyFiles = E100B.ndis4.CopyFiles

; NDIS3
[E100B.ndis3]
CopyFiles = E100B.ndis3.CopyFiles

;--- Copy files
;
[DestinationDirs]
DefaultDestDir            = 11

[SourceDisksNames]
1 = %DISKNAME%,,,

[SourceDisksFiles]
e100b9x.din = 1
8255indi.dll = 1
wol558.vxd   = 1
e100bnt5.sys = 1
e100bnt.sys  = 1
e100b.sys    = 1
8255xDel.exe = 1

; Install NDI Helper Dll
[E100B.ndi.copyfiles]
8255indi.dll,,,2
e100bnt5.sys,,,2
WOL558.vxd,,,2
8255xDel.exe,,,2
e100b9x.din,,,2

[E100B.ndis5.CopyFiles]
e100bnt5.sys,,,2
WOL558.vxd,,,2

[E100B.ndis4.CopyFiles]
e100bnt.sys,,,2

[E100B.ndis3.CopyFiles]
e100b.sys,,,2

[SpeedDpx.DelReg]
HKR,Ndi\Params\Speed
HKR,Ndi\Params\ForceDpx
HKR,Ndi\Params\PacketTagging
HKR,,Speed
HKR,,ForceDpx
HKR,,PacketTagging

;--- Localizable Strings
;
[Strings]
; Vendors
V_INTEL="Intel"

; Source disk name
DISKNAME="Intel PRO Adapter CD-ROM or floppy disk"

; Parameters
AutoDetect               = "Auto Detect"
SpeedDuplex              = "Link Speed & Duplex"
10Mb-Half-Duplex         = "10Mbps/Half Duplex"
10Mb-Full-Duplex         = "10Mbps/Full Duplex"
100Mb-Half-Duplex        = "100Mbps/Half Duplex"
100Mb-Full-Duplex        = "100Mbps/Full Duplex"
None                     = "None"
IPSecEnabled             = "Offload IP Security"
Enabled                  = "Enabled"
Disabled                 = "Disabled"
Checksum_str             = "Checksum"
OSControlled             = "OS Controlled"
Forced                   = "Forced"
WakeOnLinkSettings       = "Wake On Link Settings"
WakeOnLinkHelp           = "Allows wake-up from APM power management when link is reconnected."
TaskOffload              = "Offloading"
SecurityAssociations     = "Security Associations"

; Device descriptions
PCIE100B.DeviceDesc       = "Intel(R) PRO/100 Network Connection"
PCIE100BTX.DeviceDesc     = "Intel(R) PRO/100B PCI Adapter (TX)"
PCIE100BT4.DeviceDesc     = "Intel(R) PRO/100B PCI Adapter (T4)"
PCIE10PPCI.DeviceDesc     = "Intel(R) PRO/10+ PCI Adapter"
PCIE100RWU.DeviceDesc     = "Intel(R) PRO/100 WfM PCI Adapter"
I557IFE.DeviceDesc        = "Intel 82557-based Integrated Ethernet PCI (10/100)"
I557IFEWFM.DeviceDesc     = "82557-based Integrated Ethernet with Wake on LAN"
I558IFE.DeviceDesc        = "Intel 82558-based Integrated Ethernet"
I558IFEWFM.DeviceDesc     = "Intel 82558-based Integrated Ethernet with Wake on LAN"
PCIE100PLUS.DeviceDesc    = "Intel(R) PRO/100+ PCI Adapter"
PCIE100MAN.DeviceDesc     = "Intel(R) PRO/100+ Management Adapter"
PCIE100SERVER.DeviceDesc  = "Intel(R) PRO/100+ Server Adapter"
PCIE100SERVERW.DeviceDesc = "Intel(R) PRO/100+ Server Adapter (PILA8470B)"
PCIE100DUAL.DeviceDesc    = "Intel(R) PRO/100+ Dual Port Server Adapter"
PCIE100AOL.DeviceDesc     = "Intel(R) PRO/100+ Alert on LAN* 2 Management Adapter"
PCIE100MANAOL.DeviceDesc  = "Intel(R) PRO/100+ Alert on LAN* Management Adapter"
PCIE100MANAOLGC.DeviceDesc= "Intel(R) PRO/100+ Management Adapter with Alert On LAN* GC"
PCIE100MANAOLGS.DeviceDesc= "Intel(R) PRO/100+ Management Adapter with Alert On LAN* G Server"
I559CLONPCI.DeviceDesc    = "Intel(R) PRO/100 S Mobile LAN on Motherboard"
I559IFE.DeviceDesc        = "Intel(R) 82559 Fast Ethernet LAN on Motherboard"
I559IFEAOL.DeviceDesc     = "Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"
I559IFEAOLII.DeviceDesc   = "Intel(R) 82559 Fast Ethernet LOM with Alert on LAN* 2"
PCIE100DUALx.DeviceDesc   = "Intel(R) PRO/100 Dual Port Server Adapter"
PCIE100DUALSx.DeviceDesc  = "Intel(R) PRO/100 S Dual Port Server Adapter"
PCIE100S.DeviceDesc       = "Intel(R) PRO/100 S Management Adapter"
PCIE100SADV.DeviceDesc    = "Intel(R) PRO/100 S Advanced Management Adapter"
PCIE100SSVR.DeviceDesc    = "Intel(R) PRO/100 S Server Adapter"


PCIE100BSPLUSD.DeviceDesc = "Intel(R) PRO/100 S+ Desktop Adapter"
PCIE100S0.DeviceDesc       = "Intel(R) PRO/100 Desktop Adapter"
PCIE100Sx.DeviceDesc       = "Intel(R) PRO/100 S Desktop Adapter"
PCIE100S0SVR.DeviceDesc    = "Intel(R) PRO/100 Server Adapter"
PCIE100SxSVR.DeviceDesc    = "Intel(R) PRO/100 S Server Adapter"
PCIE100S0L.DeviceDesc      = "Intel(R) PRO/100 Network Connection"
PCIE100SxL.DeviceDesc      = "Intel(R) PRO/100 S Network Connection"
PCIE100LAVON.DeviceDesc    = "Intel(R) PRO/100 M Desktop Adapter"
PCIE100LAVONLOM.DeviceDesc = "Intel(R) PRO/100 M Network Connection"
PCIE100LAVONMB.DeviceDesc  = "Intel(R) PRO/100 M Mobile Connection"
I559IFEAOLCPQ.DeviceDesc  = "Intel(R) 82559 Fast Ethernet LOM with Alert on LAN*"

; Fujitsu Siemens Computers

HPTX.DeviceDesc    = "NetServer 10/100TX PCI LAN Adapter"

IBMFE9.DeviceDesc  = "Intel(R) 82559 Fast Ethernet LAN On Motherboard"
IBMFED.DeviceDesc  = "Intel(R) PRO/100 S Network Connection"

PCIE100BSPLUSS.DeviceDesc = "Intel(R) PRO/100 S+ Server Adapter"
PCIE100SCBRCOMBONODES.DeviceDesc= "Intel(R) PRO/100 R Mobile Combo Adapter"

Toshiba82559B.DeviceDesc     = "Intel 8255x-based Fast Ethernet"


; NT service name
e100bnt.Service.DispName = "Intel(R) PRO Adapter Driver"
