;*******************************************************************************
;*                                                                            **
;*                     I N T E L   P R O P R I E T A R Y                      **
;*                                                                            **
;*   COPYRIGHT (c) 2000-2004 BY INTEL CORPORATION. ALL RIGHTS RESERVED.  NO   **
;*   PART  OF  THIS  PROGRAM OR PUBLICATION MAY BE REPRODUCED, TRANSMITTED,   **
;*   TRANSCRIBED, STORED IN A RETRIEVAL  SYSTEM,  OR  TRANSLATED  INTO  ANY   **
;*   LANGUAGE OR COMPUTER LANGUAGE IN ANY FORM OR BY ANY MEANS, ELECTRONIC,   **
;*   MECHANICAL, MAGNETIC, OPTICAL, CHEMICAL, MANUAL, OR OTHERWISE, WITHOUT   **
;*   THE PRIOR WRITTEN PERMISSION OF :                                        **
;*                                                                            **
;*                             INTEL CORPORATION                              **
;*                                                                            **
;*                          2200 MISSION COLLEGE BLVD                         **
;*                                                                            **
;*                     SANTA CLARA, CALIFORNIA 95052-8119                     **
;*                                                                            **
;*******************************************************************************
;
;*******************************************************************************
; NET55a9x.INF
; $Revision: 30 $
;
; Intel 8255x-based PCI Ethernet Adapters
; PnP install script for Windows 9x
;   Version 7.1.12.0

[Version]
Signature       = "$Chicago$"
Class           = Net
ClassGUID       = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider        = %V_INTEL%
;CatalogFile     = e100b9xa.cat
DriverVer       = 02/10/2004,7.1.12.0


[Manufacturer]
%V_INTEL%   = Intel

[ControlFlags]
ExcludeFromSelect =  \
                        PCI\VEN_8086&DEV_2449,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_30108086,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_30118086,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_30128086,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_30138086,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_30148086,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_30158086,\
                        PCI\VEN_8086&DEV_1031,\
                        PCI\VEN_8086&DEV_1032,\
                        PCI\VEN_8086&DEV_1033,\
                        PCI\VEN_8086&DEV_1034,\
                        PCI\VEN_8086&DEV_1035,\
                        PCI\VEN_8086&DEV_1036,\
                        PCI\VEN_8086&DEV_1038,\
                        PCI\VEN_8086&DEV_1039,\
                        PCI\VEN_8086&DEV_103A,\
                        PCI\VEN_8086&DEV_103B,\
                        PCI\VEN_8086&DEV_103C,\
                        PCI\VEN_8086&DEV_103D,\
                        PCI\VEN_8086&DEV_103E,\
                        PCI\VEN_8086&DEV_1050,\
                        PCI\VEN_8086&DEV_1051,\
                        PCI\VEN_8086&DEV_1052,\
                        PCI\VEN_8086&DEV_1053,\
                        PCI\VEN_8086&DEV_1054,\
                        PCI\VEN_8086&DEV_1055,\
			PCI\VEN_8086&DEV_1064,\
			PCI\VEN_8086&DEV_1065,\
			PCI\VEN_8086&DEV_1066,\
			PCI\VEN_8086&DEV_1067,\
			PCI\VEN_8086&DEV_1068,\
			PCI\VEN_8086&DEV_1069,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_00120E11,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_01CE1014,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_01DC1014,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_01EB1014,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_01EC1014,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_02021014,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_02051014,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_02171014,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_02651014,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_02671014,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_026A1014,\
                        PCI\VEN_8086&DEV_2449&SUBSYS_00120E11,\
                        PCI\VEN_8086&DEV_2459,\
                        PCI\VEN_8086&DEV_245D



[Intel]
; DisplayName                Section        DeviceID
; -----------                -------        --------
; ich2
%PCIE100EMBLON.DeviceDesc%       = D110KMP.ndi,  PCI\VEN_8086&DEV_2449
%PCIE100EMBEDDED.DeviceDesc%     = D110K.ndi,    PCI\VEN_8086&DEV_2449&SUBSYS_30108086
%PCIE100PLUSEMBEDDED.DeviceDesc% = D110K.ndi,    PCI\VEN_8086&DEV_2449&SUBSYS_30118086
%PCIE1EMBEDDED.DeviceDesc%       = D110G.ndi,    PCI\VEN_8086&DEV_2449&SUBSYS_30128086

%PCIE100EMBLOM.DeviceDesc%       = D110K.ndi,    PCI\VEN_8086&DEV_2449&SUBSYS_30138086
%PCIE100PLUSEMBLOM.DeviceDesc%   = D110K.ndi,    PCI\VEN_8086&DEV_2449&SUBSYS_30148086

%PCIE100EMBLON.DeviceDesc%       = D110KMP.ndi,  PCI\VEN_8086&DEV_2449&SUBSYS_30188086


;ICH3 - kinerreth (9)LOM/(A)CNR/(B)+LOM/(C)+CNR/(D)LOM mobile/(E)+ Mobile
%PCIE100EMBLOM.DeviceDesc%	 = D110K.ndi,    PCI\VEN_8086&DEV_1031&SUBSYS_9550107B
%PCIE100EMBLOM.DeviceDesc%	 = D110K.ndi,    PCI\VEN_8086&DEV_1031&SUBSYS_5350107B
%PCIE100EMBLOM.DeviceDesc%	 = D110K.ndi,    PCI\VEN_8086&DEV_1031&SUBSYS_1450107B
%PCIE100EMBLOM.DeviceDesc%	 = D110K.ndi,    PCI\VEN_8086&DEV_1031&SUBSYS_0400107B
%PCIE100EMBLOM.DeviceDesc%	 = D110K.ndi,    PCI\VEN_8086&DEV_1031&SUBSYS_0401107B
%PCIE100EMBLOM.DeviceDesc%	 = D110K.ndi,    PCI\VEN_8086&DEV_1031&SUBSYS_0600107B

;ICH3
%PCIE100EMBLOM.DeviceDesc%       = D110KMP.ndi,  PCI\VEN_8086&DEV_1031
%PCIE100EMBLOM.DeviceDesc%       = D110KMP.ndi,  PCI\VEN_8086&DEV_1032
%PCIE100PLUSEMBLOM.DeviceDesc%   = D110KMP.ndi,  PCI\VEN_8086&DEV_1033
%PCIE100PLUSEMBLOM.DeviceDesc%   = D110KMP.ndi,  PCI\VEN_8086&DEV_1034
%PCIE100PLUSEMBLOM.DeviceDesc%   = D110KMP.ndi,  PCI\VEN_8086&DEV_1038

;ICH4 - kinerreth (9)LOM/(A)CNR/(B)+LOM/(C)+CNR/(D)LOM mobile/(E)+ Mobile
%PCIE100EMBLOM.DeviceDesc%       = D110K.ndi,    PCI\VEN_8086&DEV_1039
%PCIE100EMBLOM.DeviceDesc%	 = D110K.ndi,    PCI\VEN_8086&DEV_1039&SUBSYS_1049107B
%PCIE100EMBLOM.DeviceDesc%	 = D110K.ndi,    PCI\VEN_8086&DEV_1039&SUBSYS_4000107B
%PCIE100EMBLOM.DeviceDesc%	 = D110K.ndi,    PCI\VEN_8086&DEV_1039&SUBSYS_2000107B
%PCIE100EMBLOM.DeviceDesc%	 = D110K.ndi,    PCI\VEN_8086&DEV_1039&SUBSYS_2700107B
%PCIE100EMBLOM.DeviceDesc%	 = D110K.ndi,    PCI\VEN_8086&DEV_1039&SUBSYS_5288107B
%PCIE100EMBLOM.DeviceDesc%	 = D110K.ndi,    PCI\VEN_8086&DEV_1039&SUBSYS_2009107B
%PCIE100EMBLOM.DeviceDesc%	 = D110K.ndi,    PCI\VEN_8086&DEV_1039&SUBSYS_2010107B
%PCIE100EMBLOM.DeviceDesc%	 = D110K.ndi,    PCI\VEN_8086&DEV_1039&SUBSYS_2018107B
%PCIE100EMBLOM.DeviceDesc%	 = D110K.ndi,    PCI\VEN_8086&DEV_1039&SUBSYS_2019107B
%PCIE100EMBLOM.DeviceDesc%	 = D110K.ndi,    PCI\VEN_8086&DEV_1039&SUBSYS_5350107B
%PCIE100EMBLOM.DeviceDesc%       = D110K.ndi,    PCI\VEN_8086&DEV_103A
%PCIE100PLUSEMBLOM.DeviceDesc%   = D110K.ndi,    PCI\VEN_8086&DEV_103B
%PCIE100PLUSEMBLOM.DeviceDesc%   = D110K.ndi,    PCI\VEN_8086&DEV_103C
%PCIE100EMBLOM.DeviceDesc%       = D110KMP.ndi,  PCI\VEN_8086&DEV_103D
%PCIE100EMBLOM.DeviceDesc%	 = D110K.ndi,    PCI\VEN_8086&DEV_103D&SUBSYS_0402107B
%PCIE100EMBLOM.DeviceDesc%	 = D110K.ndi,    PCI\VEN_8086&DEV_103D&SUBSYS_0450107B
%PCIE100EMBLOM.DeviceDesc%	 = D110K.ndi,    PCI\VEN_8086&DEV_103D&SUBSYS_0601107B

%PCIE100PLUSEMBLOM.DeviceDesc%   = D110KMP.ndi,  PCI\VEN_8086&DEV_103E

;ICH5 - kinerreth (0)LOM/(1)CNR/(2)+LOM/(3)+CNR/(4)LOM mobile/(5)+ Mobile
%PCIE100EMBLOM.DeviceDesc%      = D110K.ndi,    PCI\VEN_8086&DEV_1050
%PCIE100EMBLOM.DeviceDesc%      = D110K.ndi,    PCI\VEN_8086&DEV_1051
%PCIE100PLUSEMBLOM.DeviceDesc%  = D110K.ndi,    PCI\VEN_8086&DEV_1052
%PCIE100PLUSEMBLOM.DeviceDesc%  = D110K.ndi,    PCI\VEN_8086&DEV_1053
%PCIE100EMBLOM.DeviceDesc%      = D110KMP.ndi,  PCI\VEN_8086&DEV_1054  ;mobile
%PCIE100PLUSEMBLOM.DeviceDesc%  = D110KMP.ndi,  PCI\VEN_8086&DEV_1055  ;mobile

;ICH6 - kinerreth (4)LOM/(5)CNR/(6)+LOM/(7)+CNR/(8)LOM mobile/(9)+ Mobile
%PCIE100EMBLOM.DeviceDesc%      = D110K.ndi,    PCI\VEN_8086&DEV_1064
%PCIE100EMBLOM.DeviceDesc%      = D110K.ndi,    PCI\VEN_8086&DEV_1065
%PCIE100PLUSEMBLOM.DeviceDesc%  = D110K.ndi,    PCI\VEN_8086&DEV_1066
%PCIE100PLUSEMBLOM.DeviceDesc%  = D110K.ndi,    PCI\VEN_8086&DEV_1067
%PCIE100EMBLOM.DeviceDesc%      = D110KMP.ndi,  PCI\VEN_8086&DEV_1068  ;mobile
%PCIE100PLUSEMBLOM.DeviceDesc%  = D110KMP.ndi,  PCI\VEN_8086&DEV_1069  ;mobile

%PCIE100PLUSEMBLOM.DeviceDesc%   = D110K.ndi,    PCI\VEN_8086&DEV_2449&SUBSYS_00120E11
%PCIE100EMBLOM.DeviceDesc%       = D110K.ndi,    PCI\VEN_8086&DEV_2449&SUBSYS_00910E11


%IBMFEK.DeviceDesc%              = D110K.ndi,    PCI\VEN_8086&DEV_2449&SUBSYS_01CE1014
%IBMFEK.DeviceDesc%              = D110K.ndi,    PCI\VEN_8086&DEV_2449&SUBSYS_01DC1014
%IBMFEK.DeviceDesc%              = D110K.ndi,    PCI\VEN_8086&DEV_2449&SUBSYS_01EB1014
%IBMFEK.DeviceDesc%              = D110K.ndi,    PCI\VEN_8086&DEV_2449&SUBSYS_01EC1014
%IBMFEK.DeviceDesc%              = D110K.ndi,    PCI\VEN_8086&DEV_2449&SUBSYS_02021014
%IBMFEK.DeviceDesc%              = D110K.ndi,    PCI\VEN_8086&DEV_2449&SUBSYS_02051014
%IBMFEK.DeviceDesc%              = D110K.ndi,    PCI\VEN_8086&DEV_2449&SUBSYS_02171014
%IBMFEK.DeviceDesc%              = D110K.ndi,    PCI\VEN_8086&DEV_2449&SUBSYS_02341014

%IBMFEK.DeviceDesc%              = D110K.ndi,    PCI\VEN_8086&DEV_2449&SUBSYS_023D1014
%IBMFEK.DeviceDesc%              = D110K.ndi,    PCI\VEN_8086&DEV_2449&SUBSYS_02441014
%IBMFEK.DeviceDesc%              = D110K.ndi,    PCI\VEN_8086&DEV_2449&SUBSYS_02451014
%IBMFEK.DeviceDesc%              = D110K.ndi,    PCI\VEN_8086&DEV_2449&SUBSYS_02651014
%IBMFEK.DeviceDesc%              = D110K.ndi,    PCI\VEN_8086&DEV_2449&SUBSYS_02671014
%IBMFEK.DeviceDesc%              = D110K.ndi,    PCI\VEN_8086&DEV_2449&SUBSYS_026A1014
%IBMFES.DeviceDesc%              = D110KMP.ndi,  PCI\VEN_8086&DEV_1031&SUBSYS_022D1014
%PCIE100EMBLOM.DeviceDesc%       = D110KMP.ndi,  PCI\VEN_8086&DEV_1031&SUBSYS_02091014
%PCIE100EMBLOM.DeviceDesc%       = D110KMP.ndi,  PCI\VEN_8086&DEV_103D&SUBSYS_05221014

; CICH support for embedded dual kinnereth
%PCIE100CICHEMBEDDED.DeviceDesc% = D110K.ndi,    PCI\VEN_8086&DEV_2459
%PCIE100CICHEMBEDDED.DeviceDesc% = D110K.ndi,    PCI\VEN_8086&DEV_245D

; The following NEC devices defined by PCI\VEN_8086&DEV_1031
;       PCI\VEN_8086&DEV_1031&SUBSYS_81691033
;       PCI\VEN_8086&DEV_1031&SUBSYS_81831033
;       PCI\VEN_8086&DEV_1031&SUBSYS_818b1033
;       PCI\VEN_8086&DEV_1031&SUBSYS_818c1033

;--- D110 Ethernet
;
[D110K.ndi]
DriverVer       = 03/04/2003,7.0.26.0
DelReg          = 82558BDelReg.DelReg
AddReg          = Speed100.reg,ICH2.reg,Kinnereth.reg, EnablePME.reg,AcpiWol.reg, e100b.ndi.reg, 82558B.reg, PowerSave.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- D110 Ethernet Mobile
;
[D110KMP.ndi]
DriverVer       = 03/04/2003,7.0.26.0
DelReg          = 82558BDelReg.DelReg
AddReg          = Speed100.reg,ICH2.reg,Kinnereth.reg, EnablePME.reg,AcpiWol.reg, e100b.ndi.reg, EnableLLPD.reg, PowerSave.reg, 82558B.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- D110 Phoneline
;
[D110G.ndi]
DriverVer       = 03/04/2003,7.0.26.0
AddReg          = Phone.reg,ICH2.reg,Gilad.reg, Gilad98.reg, e100b.ndi.reg, LogLinkState.reg
CopyFiles       = E100B.ndi.copyfiles

;--- Common 82557 NDI parameters
;
[82557.reg]
HKR,Ndi\Params\NumRfd,                ParamDesc,  0, "Receive Buffers"
HKR,Ndi\Params\NumRfd,                Type,       0, "int"
HKR,Ndi\Params\NumRfd,                Default,    0, "48"
HKR,Ndi\Params\NumRfd,                Min,        0, "8"
HKR,Ndi\Params\NumRfd,                Max,        0, "1024"
HKR,Ndi\Params\NumRfd,                Step,       0, "1"
HKR,Ndi\Params\NumRfd,                Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\NumRfd,   MiniHelp,   0, "Number of buffers used by the driver when copying data to the protocol memory."

HKR,Ndi\Params\NumTcb,                ParamDesc,  0, "Transmit Control Blocks"
HKR,Ndi\Params\NumTcb,                Type,       0, "int"
HKR,Ndi\Params\NumTcb,                Default,    0, "16"
HKR,Ndi\Params\NumTcb,                Min,        0, "8"
HKR,Ndi\Params\NumTcb,                Max,        0, "64"
HKR,Ndi\Params\NumTcb,                Step,       0, "1"
HKR,Ndi\Params\NumTcb,                Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\NumTcb,   MiniHelp,   0, "Sets the number of control blocks available for adapter use."

HKR,Ndi\Params\NumCoalesce,           ParamDesc,  0, "Coalesce Buffers"
HKR,Ndi\Params\NumCoalesce,           Type,       0, "int"
HKR,Ndi\Params\NumCoalesce,           Default,    0, "8"
HKR,Ndi\Params\NumCoalesce,           Min,        0, "1"
HKR,Ndi\Params\NumCoalesce,           Max,        0, "32"
HKR,Ndi\Params\NumCoalesce,           Step,       0, "1"
HKR,Ndi\Params\NumCoalesce,           Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\NumCoalesce, MiniHelp, 0, "Number of buffers available for transmits acceleration."

HKR,Ndi\Params\Adaptive_IFS,          ParamDesc,  0, "Adaptive Inter-Frame Spacing"
HKR,Ndi\Params\Adaptive_IFS,          Type,       0, "int"
HKR,Ndi\Params\Adaptive_IFS,          Default,    0, "1"
HKR,Ndi\Params\Adaptive_IFS,          Min,        0, "0"
HKR,Ndi\Params\Adaptive_IFS,          Max,        0, "255"
HKR,Ndi\Params\Adaptive_IFS,          Step,       0, "1"
HKR,Ndi\Params\Adaptive_IFS,          Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\Adaptive_IFS, MiniHelp, 0, "Compensates for excessive Ethernet packet collisions."

HKR,Ndi\Params\Threshold,             ParamDesc,  0, "Adaptive Transmit Threshold"
HKR,Ndi\Params\Threshold,             Type,       0, "int"
HKR,Ndi\Params\Threshold,             Default,    0, "200"
HKR,Ndi\Params\Threshold,             Min,        0, "0"
HKR,Ndi\Params\Threshold,             Max,        0, "200"
HKR,Ndi\Params\Threshold,             Step,       0, "1"
HKR,Ndi\Params\Threshold,             Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\Threshold, MiniHelp,  0, "Sets number of bytes before adapter empties its FIFO buffer. Actual value is 8 times setting."

HKR,Ndi\Params\HPQPriorityLevel,             ParamDesc,  0, "Priority Level Definition"
HKR,Ndi\Params\HPQPriorityLevel,             Type,       0, "int"
HKR,Ndi\Params\HPQPriorityLevel,             Default,    0, "4"
HKR,Ndi\Params\HPQPriorityLevel,             Min,        0, "0"
HKR,Ndi\Params\HPQPriorityLevel,             Max,        0, "7"
HKR,Ndi\Params\HPQPriorityLevel,             Step,       0, "1"
HKR,Ndi\Params\HPQPriorityLevel,             Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\HPQPriorityLevel, MiniHelp,  0, "Sets the controlled cutoff level for using HPQ."

HKR,Ndi\Params\UcodeSW,               ParamDesc,  0, "Adaptive Technology"
HKR,Ndi\Params\UcodeSW,               Type,       0, "enum"
HKR,Ndi\Params\UcodeSW,               Default,    0, "1"
HKR,Ndi\Params\UcodeSW\Enum,          "1",        0, "On"
HKR,Ndi\Params\UcodeSW\Enum,          "0",        0, "Off"
HKR,PROSetNdi\NdiExt\Params\UcodeSW,  MiniHelp,   0, "Enables/Disables the Adaptive Technology performance feature."

HKR,Ndi\Params\Coalesce,              ParamDesc,  0, "PCI Bus Efficiency"
HKR,Ndi\Params\Coalesce,              Type,       0, "enum"
HKR,Ndi\Params\Coalesce,              Default,    0, "0"
HKR,Ndi\Params\Coalesce\Enum,         "1",        0, "Enabled"
HKR,Ndi\Params\Coalesce\Enum,         "0",        0, "Disabled"
HKR,PROSetNdi\NdiExt\Params\Coalesce, MiniHelp,   0, "Coalesces transmit packets into single buffer before sending them to network. "

HKR,Ndi\Params\AlwaysConnectGoal,              ParamDesc,  0, "Low Resource Connectivity"
HKR,Ndi\Params\AlwaysConnectGoal,              Type,       0, "enum"
HKR,Ndi\Params\AlwaysConnectGoal,              Default,    0, "1"
HKR,Ndi\Params\AlwaysConnectGoal\Enum,         "1",        0, "Enabled"
HKR,Ndi\Params\AlwaysConnectGoal\Enum,         "0",        0, "Disabled"
HKR,PROSetNdi\NdiExt\Params\AlwaysConnectGoal, MiniHelp,   0,  "Try to load the driver in low resources environment."

HKR,Ndi\Params\NetworkAddress,  ParamDesc,  0, "Locally Administered Address"
HKR,Ndi\Params\NetworkAddress,  Type,       0, "edit"
HKR,Ndi\Params\NetworkAddress,  Default,    0, "0"
HKR,NDI\params\NetworkAddress,  LimitText,  0, "12"
HKR,NDI\params\NetworkAddress,  UpperCase,  0, "1"
HKR,PROSetNdi\NdiExt\Params\NetworkAddress,  MiniHelp,   0, "By default, an address is not present and the value field is left blank. To set a LAA in Intel(R) PROSet, enter one in the value field. Note: To set a LAA in Device Manager, select the Value option and enter an address in the field provided."

HKR,Ndi\Params\ConfigIFS,                ParamDesc,  0, "Retransmit Inter-Frame Spacing"
HKR,Ndi\Params\ConfigIFS,                Type,       0, "int"
HKR,Ndi\Params\ConfigIFS,                Default,    0, "6"
HKR,Ndi\Params\ConfigIFS,                Min,        0, "0"
HKR,Ndi\Params\ConfigIFS,                Max,        0, "15"
HKR,Ndi\Params\ConfigIFS,                Step,       0, "1"
HKR,Ndi\Params\ConfigIFS,                Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\ConfigIFS,   MiniHelp,   0, "Compensates for excessive Ethernet packet collisions by controlling retransmit timing."

HKR,,PcNic,                     0, "1"
HKR,,MWIEnable,                 2, "0"
HKR,,AdaptiveStalledInterrupts, 2, "1"
HKR,,AdaptiveCarrierLoss,       2, "1"
HKR,,AdaptiveTransmitMethod,    2, "1"
HKR,,Threshold,                 0, "200"

HKR,,DeviceVxDsPrefix,          0, "e100b"

;--- 82558 ACPI Wake On LAN parameter
;
[AcpiWol.reg]
HKR,Ndi\Params\AcpiWol,               ParamDesc,  0, "ACPI Wake On LAN"
HKR,Ndi\Params\AcpiWol,               Type,       0, "enum"
HKR,Ndi\Params\AcpiWol,               Default,    0, "1"
HKR,Ndi\Params\AcpiWol\Enum,          "1",        0, "Enabled"
HKR,Ndi\Params\AcpiWol\Enum,          "0",        0, "Disabled"
HKR,PROSetNdi\NdiExt\Params\AcpiWol,  MiniHelp,   0, "Enables or disables the Magic Packet* service for Wake On LAN with Windows 98 version 4.10.1998."

HKLM,System\CurrentControlSet\Services\VxD\ACPIWOL,Start,     1, 00
HKLM,System\CurrentControlSet\Services\VxD\ACPIWOL,StaticVxD, 0, "WOL558.vxd"

;--- Log Link State Event
;
[LogLinkState.reg]
HKR,,LogLinkStateEvent, 0,      "1"

;--- 82558 specifics
;
[82558.reg]
; 802.1p/802.1q Packet Tagging   - This parameter repeated in ICH2.REG
HKR,Ndi\Params\TaggingMode,         ParamDesc,  0, "QoS Packet Tagging"
HKR,Ndi\Params\TaggingMode,         Type,       0, "enum"
HKR,Ndi\Params\TaggingMode,         Default,    0, "0"
HKR,Ndi\Params\TaggingMode\Enum,    "1",        0, %Enabled%
HKR,Ndi\Params\TaggingMode\Enum,    "0",        0, %Disabled%
HKR,PROSetNdi\NdiExt\Params\TaggingMode, MiniHelp, 0, "Send and receive IEEE Tagged frames (802.3ac/802.1p/802.1Q)."

HKR,Ndi\Params\FlowControl,              ParamDesc,  0, "Flow Control Settings"
HKR,Ndi\Params\FlowControl,              Type,       0, "enum"
HKR,Ndi\Params\FlowControl,              Default,    0, "3"
HKR,Ndi\Params\FlowControl\Enum,         "3",        0, "Generate and Respond"
HKR,Ndi\Params\FlowControl\Enum,         "2",        0, "Respond"
HKR,Ndi\Params\FlowControl\Enum,         "1",        0, "Generate"
HKR,Ndi\Params\FlowControl\Enum,         "0",        0, "Off"
HKR,PROSetNdi\NdiExt\Params\FlowControl, MiniHelp,   0, "Pauses packet transmission on receipt of full flow control frame and Send full flow control frame to notify the other side to stop transmission."
HKR,,				   	FlowControl, 0, "3"

; Adaptive Performance Tuning
HKR,PROSetNdi\Params\CPUSaver,        ParamDesc,  0, "Adaptive Performance Tuning"
HKR,PROSetNdi\Params\CPUSaver,        Type,       0, "slider"
HKR,PROSetNdi\Params\CPUSaver,        Default,    0, "1536"
HKR,,CPUSaver,                                    0, "1536"
HKR,PROSetNdi\Params\CPUSaver,        LeftLabel,  0, "Adapter Bandwidth"
HKR,PROSetNdi\Params\CPUSaver,        RightLabel, 0, "CPU Utilization"
HKR,PROSetNdi\Params\CPUSaver,        MiniHelp,   0, "Sets optimal point of CPU/Adapter performance for this system.  See help."
HKR,PROSetNdi\Params\CPUSaver\Values, "0",        0, "0"
HKR,PROSetNdi\Params\CPUSaver\Values, "1",        0, "1"
HKR,PROSetNdi\Params\CPUSaver\Values, "2",        0, "512"
HKR,PROSetNdi\Params\CPUSaver\Values, "3",        0, "768"
HKR,PROSetNdi\Params\CPUSaver\Values, "4",        0, "1024"
HKR,PROSetNdi\Params\CPUSaver\Values, "5",        0, "1280"
HKR,PROSetNdi\Params\CPUSaver\Values, "6",        0, "1536"
HKR,PROSetNdi\Params\CPUSaver\Values, "7",        0, "1792"
HKR,PROSetNdi\Params\CPUSaver\Values, "8",        0, "2048"
HKR,PROSetNdi\Params\CPUSaver\Values, "9",        0, "2304"
HKR,PROSetNdi\Params\CPUSaver\Values, "10",       0, "2560"
HKR,PROSetNdi\Params\CPUSaver\Values, "11",       0, "2816"
HKR,PROSetNdi\Params\CPUSaver\Values, "12",       0, "3072"
HKR,PROSetNdi\Params\CPUSaver\Values, "13",       0, "3328"
HKR,PROSetNdi\Params\CPUSaver\Values, "14",       0, "3584"
HKR,PROSetNdi\Params\CPUSaver\Values, "15",       0, "3840"
HKR,PROSetNdi\Params\CPUSaver\Values, "16",       0, "4096"

;--- 82558 B Rev 5
;
[82558B.reg]
; WakeOn
HKR, Ndi\Params\WakeOn,       	  ParamDesc,          0, "Wake on Settings"
HKR, Ndi\Params\WakeOn,       	  default,            0, "246"
HKR, Ndi\Params\WakeOn\Enum,  	  "0",                0, %Disabled%
HKR, Ndi\Params\WakeOn\Enum,  	  "6",                0, "Wake on Magic Packet"
HKR, Ndi\Params\WakeOn\Enum,  	  "116",              0, "Wake on directed packet"
HKR, Ndi\Params\WakeOn\Enum,  	  "118",              0, "Wake on Magic & Directed"
HKR, Ndi\Params\WakeOn\Enum,      "246",              0, %OSControlled%
HKR, Ndi\Params\WakeOn,       	  type,               0, "enum"
HKR, Ndi\Params\WakeOn,       	  ExposeLevel,        0, "2"
HKR, Ndi\Params\WakeOn,       	  MiniHelp,           0, "Determines which packets can be enabled to Wake up the system (Direct Packets, Magic Packet etc.)."
HKR,,				  WakeOn, 	      0, "246"

;Wake on Link parameter
HKR, Ndi\Params\WakeOnLink,       ParamDesc,          0, %WakeOnLinkSettings%
HKR, Ndi\Params\WakeOnLink\Enum,  "0",                0, %Disabled%
HKR, Ndi\Params\WakeOnLink\Enum,  "1",                0, %OSControlled% 
HKR, Ndi\Params\WakeOnLink\Enum,  "2",                0, %Forced%
HKR, Ndi\Params\WakeOnLink,       type,               0, "enum"
;HKR, Ndi\Params\WakeOnLink,       ExposeLevel,        0, "2"
HKR, PROSetNdi\NdiExt\Params\WakeOnLink, MiniHelp,    0, %WakeOnLinkHelp% 

;--- 82559 Enable PME
;
[EnablePME.reg]
HKR,Ndi\Params\EnablePME,             ParamDesc,  0, "Enable PME"
HKR,Ndi\Params\EnablePME,             Type,       0, "enum"
HKR,Ndi\Params\EnablePME,             Default,    0, "2"
HKR,Ndi\Params\EnablePME\Enum,        "1",        0, "Enabled"
HKR,Ndi\Params\EnablePME\Enum,        "0",        0, "Disabled"
HKR,Ndi\Params\EnablePME\Enum,        "2",        0, "No Action"
HKR,Ndi\Params\EnablePME\Enum,        "255",      0, "Hardware Default"
HKR,PROSetNdi\NdiExt\Params\EnablePME, MiniHelp,  0, "Allows wake-up from APM power management when enabled. Disable shuts down LAN controller under ACPI"

;--- Expose Power Mangement feature in Lavon
[PowerSave.reg]
HKR,,AutoPowerSaveModeEnabled, 0, "1"
HKR,,Force10MbOnD3, 0, "1"
HKR,,SavePowerNowEnabled,    0, "1"

[ICH2.reg]
; 802.1p/802.1q Packet Tagging   - This parameter repeated in 82558.REG
HKR,Ndi\Params\TaggingMode,         ParamDesc,  0, "QoS Packet Tagging"
HKR,Ndi\Params\TaggingMode,         Type,       0, "enum"
HKR,Ndi\Params\TaggingMode,         Default,    0, "0"
HKR,Ndi\Params\TaggingMode\Enum,    "1",        0, "Enabled"
HKR,Ndi\Params\TaggingMode\Enum,    "0",        0, "Disabled"
HKR,PROSetNdi\NdiExt\Params\TaggingMode, MiniHelp, 0, "Send and receive IEEE Tagged frames (802.3ac/802.1p/802.1Q)."

; Flow Control Settings
HKR,Ndi\Params\FlowControl,              ParamDesc,  0, "Flow Control Settings"
HKR,Ndi\Params\FlowControl,              Type,       0, "enum"
HKR,Ndi\Params\FlowControl,              Default,    0, "3"
HKR,Ndi\Params\FlowControl\Enum,         "3",        0, "Generate and Respond"
HKR,Ndi\Params\FlowControl\Enum,         "2",        0, "Respond"
HKR,Ndi\Params\FlowControl\Enum,         "1",        0, "Generate"
HKR,Ndi\Params\FlowControl\Enum,         "0",        0, "Off"
HKR,PROSetNdi\NdiExt\Params\FlowControl, MiniHelp,   0, "Pauses packet transmission on receipt of full flow control frame and Send full flow control frame to notify the other side to stop transmission."

HKR,Ndi\Params\NumRfd,                ParamDesc,  0, "Receive Buffers"
HKR,Ndi\Params\NumRfd,                Type,       0, "int"
HKR,Ndi\Params\NumRfd,                Default,    0, "48"
HKR,Ndi\Params\NumRfd,                Min,        0, "8"
HKR,Ndi\Params\NumRfd,                Max,        0, "1024"
HKR,Ndi\Params\NumRfd,                Step,       0, "1"
HKR,Ndi\Params\NumRfd,                Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\NumRfd,   MiniHelp,   0, "Number of buffers used by the driver when copying data to the protocol memory."

HKR,Ndi\Params\NumTcb,                ParamDesc,  0, "Transmit Control Blocks"
HKR,Ndi\Params\NumTcb,                Type,       0, "int"
HKR,Ndi\Params\NumTcb,                Default,    0, "16"
HKR,Ndi\Params\NumTcb,                Min,        0, "8"
HKR,Ndi\Params\NumTcb,                Max,        0, "64"
HKR,Ndi\Params\NumTcb,                Step,       0, "1"
HKR,Ndi\Params\NumTcb,                Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\NumTcb,   MiniHelp,   0, "Sets the number of control blocks available for adapter use."

HKR,Ndi\Params\NumCoalesce,           ParamDesc,  0, "Coalesce Buffers"
HKR,Ndi\Params\NumCoalesce,           Type,       0, "int"
HKR,Ndi\Params\NumCoalesce,           Default,    0, "8"
HKR,Ndi\Params\NumCoalesce,           Min,        0, "1"
HKR,Ndi\Params\NumCoalesce,           Max,        0, "32"
HKR,Ndi\Params\NumCoalesce,           Step,       0, "1"
HKR,Ndi\Params\NumCoalesce,           Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\NumCoalesce, MiniHelp, 0, "Number of buffers available for transmits acceleration."

HKR,Ndi\Params\Adaptive_IFS,          ParamDesc,  0, "Adaptive Inter-Frame Spacing"
HKR,Ndi\Params\Adaptive_IFS,          Type,       0, "int"
HKR,Ndi\Params\Adaptive_IFS,          Default,    0, "1"
HKR,Ndi\Params\Adaptive_IFS,          Min,        0, "0"
HKR,Ndi\Params\Adaptive_IFS,          Max,        0, "255"
HKR,Ndi\Params\Adaptive_IFS,          Step,       0, "1"
HKR,Ndi\Params\Adaptive_IFS,          Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\Adaptive_IFS, MiniHelp, 0, "Compensates for excessive Ethernet packet collisions."

HKR,Ndi\Params\Threshold,             ParamDesc,  0, "Adaptive Transmit Threshold"
HKR,Ndi\Params\Threshold,             Type,       0, "int"
HKR,Ndi\Params\Threshold,             Default,    0, "200"
HKR,Ndi\Params\Threshold,             Min,        0, "0"
HKR,Ndi\Params\Threshold,             Max,        0, "200"
HKR,Ndi\Params\Threshold,             Step,       0, "1"
HKR,Ndi\Params\Threshold,             Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\Threshold, MiniHelp,  0, "Sets number of bytes before adapter empties its FIFO buffer. Actual value is 8 times setting."

HKR,Ndi\Params\UcodeSW,               ParamDesc,  0, "Adaptive Technology"
HKR,Ndi\Params\UcodeSW,               Type,       0, "enum"
HKR,Ndi\Params\UcodeSW,               Default,    0, "1"
HKR,Ndi\Params\UcodeSW\Enum,          "1",        0, "On"
HKR,Ndi\Params\UcodeSW\Enum,          "0",        0, "Off"
HKR,PROSetNdi\NdiExt\Params\UcodeSW,  MiniHelp,   0, "Enables/Disables the Adaptive Technology performance feature."

HKR,Ndi\Params\Coalesce,              ParamDesc,  0, "PCI Bus Efficiency"
HKR,Ndi\Params\Coalesce,              Type,       0, "enum"
HKR,Ndi\Params\Coalesce,              Default,    0, "0"
HKR,Ndi\Params\Coalesce\Enum,         "1",        0, "Enabled"
HKR,Ndi\Params\Coalesce\Enum,         "0",        0, "Disabled"
HKR,PROSetNdi\NdiExt\Params\Coalesce, MiniHelp,   0, "Coalesces transmit packets into single buffer before sending them to network. "

; Adaptive Performance Tuning
HKR,PROSetNdi\Params\CPUSaver,        ParamDesc,  0, "Adaptive Performance Tuning"
HKR,PROSetNdi\Params\CPUSaver,        Type,       0, "slider"
HKR,PROSetNdi\Params\CPUSaver,        Default,    0, "512"
HKR,,CPUSaver,                                    0, "512"
HKR,PROSetNdi\Params\CPUSaver,        LeftLabel,  0, "Adapter Bandwidth"
HKR,PROSetNdi\Params\CPUSaver,        RightLabel, 0, "CPU Utilization"
HKR,PROSetNdi\Params\CPUSaver,        MiniHelp,   0, "Sets optimal point of CPU/Adapter performance for this system.  See help."
HKR,PROSetNdi\Params\CPUSaver\Values, "0",        0, "0"
HKR,PROSetNdi\Params\CPUSaver\Values, "1",        0, "1"
HKR,PROSetNdi\Params\CPUSaver\Values, "2",        0, "512"
HKR,PROSetNdi\Params\CPUSaver\Values, "3",        0, "768"
HKR,PROSetNdi\Params\CPUSaver\Values, "4",        0, "1024"
HKR,PROSetNdi\Params\CPUSaver\Values, "5",        0, "1280"
HKR,PROSetNdi\Params\CPUSaver\Values, "6",        0, "1536"
HKR,PROSetNdi\Params\CPUSaver\Values, "7",        0, "1792"
HKR,PROSetNdi\Params\CPUSaver\Values, "8",        0, "2048"
HKR,PROSetNdi\Params\CPUSaver\Values, "9",        0, "2304"
HKR,PROSetNdi\Params\CPUSaver\Values, "10",       0, "2560"
HKR,PROSetNdi\Params\CPUSaver\Values, "11",       0, "2816"
HKR,PROSetNdi\Params\CPUSaver\Values, "12",       0, "3072"
HKR,PROSetNdi\Params\CPUSaver\Values, "13",       0, "3328"
HKR,PROSetNdi\Params\CPUSaver\Values, "14",       0, "3584"
HKR,PROSetNdi\Params\CPUSaver\Values, "15",       0, "3840"
HKR,PROSetNdi\Params\CPUSaver\Values, "16",       0, "4096"

HKR,Ndi\Params\NetworkAddress,  ParamDesc,  0, "Locally Administered Address"
HKR,Ndi\Params\NetworkAddress,  Type,       0, "edit"
HKR,Ndi\Params\NetworkAddress,  Default,    0, "0"
HKR,NDI\params\NetworkAddress,  LimitText,  0, "12"
HKR,NDI\params\NetworkAddress,  UpperCase,  0, "1"
HKR,PROSetNdi\NdiExt\Params\NetworkAddress,  MiniHelp,   0, "Allows you to change the network address."

HKR,Ndi\Params\ConfigIFS,                ParamDesc,  0, "Retransmit Inter-Frame Spacing"
HKR,Ndi\Params\ConfigIFS,                Type,       0, "int"
HKR,Ndi\Params\ConfigIFS,                Default,    0, "10"
HKR,Ndi\Params\ConfigIFS,                Min,        0, "0"
HKR,Ndi\Params\ConfigIFS,                Max,        0, "15"
HKR,Ndi\Params\ConfigIFS,                Step,       0, "1"
HKR,Ndi\Params\ConfigIFS,                Base,       0, "10"
HKR,PROSetNdi\NdiExt\Params\ConfigIFS,   MiniHelp,   0, "Compensates for excessive Ethernet packet collisions by controlling retransmit timing."

;HKR,,Threshold,                 0, "12"         ; Adaptive Transmit Threshold
;HKR,,UcodeSW,                   0, "1"          ; Adaptive Technology
;HKR,,Adaptive_IFS,              0, "1"          ; Adaptive Inter-Frame Spacing
HKR,,TaggingMode,               0, "0"          ; Tagging mode
;HKR,,CPUSaver,                  0, "512"        ; Adaptive Performance Tuning
HKR,,PcNic,                     0, "1"
HKR,,MWIEnable,                 0, "0"
HKR,,DeviceVxDsPrefix,          0, "e100b"
HKR,,HPQDisable,                0, "1"
HKR,,AdaptiveStalledInterrupts, 2, "1"
HKR,,AdaptiveCarrierLoss,       2, "1"
HKR,,AdaptiveTransmitMethod,    2, "1"
HKR,,Threshold,                 0, "200"

;--- Kinnereth
[Kinnereth.reg]
HKR,,BroadcastEnable,           0, "1"
HKR,,EnableDynamicReducedPower, 0, "1"

[Kinnerth.DelReg]
HKR,Ndi\Params\AcpiWol
HKR,,AcpiWol

;--- Gilad parameters starts
[Gilad.reg]
HKR,,EnablePME,         0, "2"
HKR,,BroadcastEnable,   0, "0"

[Gilad98.reg]
HKLM,System\CurrentControlSet\Services\VxD\ACPIWOL,Start,     1, 00
HKLM,System\CurrentControlSet\Services\VxD\ACPIWOL,StaticVxD, 0, "WOL558.vxd"

HKR,,AcpiWol,           0, "1"  ; ACPI wake on Lan

;--- Enable Power Down
;
[EnableLLPD.reg]
HKR,Ndi\Params\EnablePowerDownOnLinkLoss,      ParamDesc,  0, "Smart Power Down"
HKR,Ndi\Params\EnablePowerDownOnLinkLoss,      Type,       0, "enum"
HKR,Ndi\Params\EnablePowerDownOnLinkLoss,      Default,    0, "1"
HKR,Ndi\Params\EnablePowerDownOnLinkLoss\Enum, "1",        0, "Enabled"
HKR,Ndi\Params\EnablePowerDownOnLinkLoss\Enum, "0",        0, "Disabled"
HKR,PROSetNdi\NdiExt\Params\EnablePowerDownOnLinkLoss, MiniHelp, 0, "Removes adapter power when LAN cable disconnected."

HKR,Ndi\Params\LinkBasedLogin,              ParamDesc,  0, "Adaptive Link Response"
HKR,Ndi\Params\LinkBasedLogin,              Type,       0, "enum"
HKR,Ndi\Params\LinkBasedLogin,              Default,    0, "0"
HKR,Ndi\Params\LinkBasedLogin\Enum,         "1",        0, "On"
HKR,Ndi\Params\LinkBasedLogin\Enum,         "0",        0, "Off"
HKR,PROSetNdi\NdiExt\Params\LinkBasedLogin, MiniHelp,   0, "Enables Adaptive Link Response to check PHYLink status."

[LLPDD_OFF.reg]
HKR,Ndi\Params\EnablePowerDownOnLinkLoss,      Default,    0, "0"


;--- CPUSaver override for Cardbus
;
[CPUSaverOverride.reg]
HKR,PROSetNdi\Params\CPUSaver,  Default,    0, "1"
HKR,,CPUSaver,                              0, "1"

;--- Speed Duplex Mode common base 10/100Mb
;
[Speed100.reg]
HKR, Ndi\params\SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR, Ndi\params\SpeedDuplex,       default,    0, "0"
HKR, Ndi\params\SpeedDuplex,       type,       0, "enum"
HKR, Ndi\params\SpeedDuplex\enum,  "0",        0, %AutoDetect%
HKR, Ndi\params\SpeedDuplex\enum,  "1",        0, %10Mb-Half-Duplex%
HKR, Ndi\params\SpeedDuplex\enum,  "2",        0, %10Mb-Full-Duplex%
HKR, Ndi\params\SpeedDuplex\enum,  "3",        0, %100Mb-Half-Duplex%
HKR, Ndi\params\SpeedDuplex\enum,  "4",        0, %100Mb-Full-Duplex%
HKR, PROSetNdi\NdiExt\params\SpeedDuplex, MiniHelp,    0, "Sets link speed to 10/100 Mbps and duplex to half or full. Must coincide with switch port or no link will occur."
HKR, PROSetNdi\NdiExt\params\SpeedDuplex, ExposeLevel, 0, "2"

;--- Gilad Phoneline
;
[Phone.reg]
HKR, Ndi\params\PhyPhonePower,       ParamDesc,  0, %PhyPhonePower%
HKR, Ndi\params\PhyPhonePower,       default,    0, "0"
HKR, Ndi\params\PhyPhonePower,       type,       0, "enum"
HKR, Ndi\params\PhyPhonePower\enum,  "0",        0, %Low%
HKR, Ndi\params\PhyPhonePower\enum,  "1",        0, %High%

HKR, Ndi\params\PhyPhoneSpeed,       ParamDesc,  0, %PhyPhoneSpeed%
HKR, Ndi\params\PhyPhoneSpeed,       default,    0, "1"
HKR, Ndi\params\PhyPhoneSpeed,       type,       0, "enum"
HKR, Ndi\params\PhyPhoneSpeed\enum,  "0",        0, %Low%
HKR, Ndi\params\PhyPhoneSpeed\enum,  "1",        0, %High%

HKR, Ndi\params\PhyGiladIfs,       ParamDesc,  0, %PhyGiladIfs%
HKR, Ndi\params\PhyGiladIfs,       default,    0, "96"
HKR, Ndi\params\PhyGiladIfs,       type,       0, "enum"
HKR, Ndi\params\PhyGiladIfs\enum,  "96",       0, " 96 bit-times"
HKR, Ndi\params\PhyGiladIfs\enum,  "112",      0, "112 bit-times"
HKR, Ndi\params\PhyGiladIfs\enum,  "128",      0, "128 bit-times"
HKR, Ndi\params\PhyGiladIfs\enum,  "144",      0, "144 bit-times"
HKR, Ndi\params\PhyGiladIfs\enum,  "160",      0, "160 bit-times"
HKR, Ndi\params\PhyGiladIfs\enum,  "176",      0, "176 bit-times"
HKR, Ndi\params\PhyGiladIfs\enum,  "192",      0, "192 bit-times"
HKR, Ndi\params\PhyGiladIfs\enum,  "208",      0, "208 bit-times"
HKR, Ndi\params\PhyGiladIfs\enum,  "224",      0, "224 bit-times"
HKR, Ndi\params\PhyGiladIfs\enum,  "240",      0, "240 bit-times"

;Remove old TaskOffload registry keys
[TaskOffload.DelReg]
HKR,Ndi\Params\TaskOffload
HKR,,TaskOffload

[82558BDelReg.DelReg]
HKR, PROSetNdi\Params\WakeOn
HKR, Ndi\Params\WakeOn
HKR, Ndi\Params\WakeOnLink

;--- Win9x NDI object registration
;
[E100B.ndi.reg]
HKR,,               DevLoader,        0, "*ndis"
HKR,,               DeviceVxDs,       0, "e100bnt5.sys"
HKR,,               EnumPropPages,    0, "netdi.dll,EnumPropPages"
HKR,,               Driver,           0, "e100bnt.sys"
HKR,NDIS,           LogDriverName,    0, "E100B"
HKR,NDIS,           MajorNdisVersion, 1, 03
HKR,NDIS,           MinorNdisVersion, 1, 0A
HKR,Ndi,            NdiInstaller,     0, "8255indi.dll,i557NdiProc"
HKR,Ndi,            DeviceID,         0, "PCI\VEN_8086&DEV_1229"
HKR,Ndi\Interfaces, DefUpper,         0, "ndis3"
HKR,Ndi\Interfaces, DefLower,         0, "ethernet"
HKR,Ndi\Interfaces, UpperRange,       0, "ndis3"
HKR,Ndi\Interfaces, LowerRange,       0, "ethernet"

;--- Uninstallation
;adapters not hardcoded to remove

HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1031, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1032, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1033, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1034, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1035, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1036, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1038, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1039, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 103A, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 103B, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 103C, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 103D, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 103E, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1050, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1051, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1052, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1053, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1054, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1055, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1064, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1065, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1066, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1067, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1068, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1069, 0, "82562"

HKLM,Software\Microsoft\Windows\CurrentVersion\Uninstall\PROSet,DisplayName, 0, "Intel(R) PRO Ethernet Adapter and Software"
HKLM,Software\Microsoft\Windows\CurrentVersion\Uninstall\PROSet,UninstallString, 0, "8255xDel.exe"
HKLM,Software\Intel\Prounstl\Dins, e100b9x.din, 0, "8255x.Uninstall"

;--- NT NDI object registration
;
[E100B.ndi.NT.reg]
HKR,Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR,Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR,Ndi,            Service,    0, "E100B"

HKR,,LogErrorMessages, 0, "1"

HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1031, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1032, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1033, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1034, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1035, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1036, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1038, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1039, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 103A, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 103B, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 103C, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 103D, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 103E, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1050, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1051, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1052, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1053, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1054, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1055, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1064, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1065, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1066, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1067, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1068, 0, "82562"
HKLM,Software\Intel\Prounstl\SupportedDevices\8086, 1069, 0, "82562"

;--- Uninstallation
HKLM,Software\Microsoft\Windows\CurrentVersion\Uninstall\PROSet,DisplayName, 0, "Intel(R) PRO Network Adapters and Drivers"
HKLM,Software\Microsoft\Windows\CurrentVersion\Uninstall\PROSet,UninstallString, 0, "Prounstl.exe"
HKLM,Software\Intel\Prounstl\Dins, e100b9x.din, 0, "8255x.Uninstall"

;--- Driver Install
;
; NDIS5
[E100B.ndis5]
CopyFiles = E100B.ndis5.CopyFiles

; NDIS4
[E100B.ndis4]
CopyFiles = E100B.ndis4.CopyFiles

; NDIS3
[E100B.ndis3]
CopyFiles = E100B.ndis3.CopyFiles

;--- Copy files
;
[DestinationDirs]
DefaultDestDir            = 11

[SourceDisksNames]
1 = %DISKNAME%,,,

[SourceDisksFiles]
e100b9x.din = 1
8255indi.dll = 1
wol558.vxd   = 1
e100bnt5.sys = 1
e100bnt.sys  = 1
e100b.sys    = 1
8255xDel.exe = 1

; Install NDI Helper Dll
[E100B.ndi.copyfiles]
8255indi.dll,,,2
e100bnt5.sys,,,2
WOL558.vxd,,,2
8255xDel.exe,,,2
e100b9x.din,,,2

[E100B.ndis5.CopyFiles]
e100bnt5.sys,,,2
WOL558.vxd,,,2

[E100B.ndis4.CopyFiles]
e100bnt.sys,,,2

[E100B.ndis3.CopyFiles]
e100b.sys,,,2

;--- Localizable Strings
;
[Strings]
; Vendors
V_INTEL="Intel"

; Source disk name
DISKNAME="Intel PRO Adapter CD-ROM or floppy disk"

; Parameters
AutoDetect               = "Auto Detect"
SpeedDuplex              = "Link Speed & Duplex"
10Mb-Half-Duplex         = "10Mbps/Half Duplex"
10Mb-Full-Duplex         = "10Mbps/Full Duplex"
100Mb-Half-Duplex        = "100Mbps/Half Duplex"
100Mb-Full-Duplex        = "100Mbps/Full Duplex"
PhyPhoneSpeed            = "Phoneline Transmit Speed"
PhyPhonePower            = "Phoneline Power Level"
PhyGiladIfs              = "Inter Frame Spacing"
High                     = "High"
Low                      = "Low"
None                     = "None"
IPSecEnabled             = "Offload IP Security"
Enabled                  = "Enabled"
Disabled                 = "Disabled"
Checksum_str             = "Checksum"
OSControlled             = "OS Controlled"
Forced                   = "Forced"
WakeOnLinkSettings       = "Wake On Link Settings"
WakeOnLinkHelp           = "Allows wake-up from APM power management when link is reconnected."
TaskOffload              = "Offloading"
SecurityAssociations     = "Security Associations"

; Device descriptions

PCIE100B.DeviceDesc            = "Intel(R) PRO/100 Network Connection"
PCIE100EMBEDDED.DeviceDesc     = "Intel(R) PRO/100 VE Desktop Adapter"
PCIE100PLUSEMBEDDED.DeviceDesc = "Intel(R) PRO/100 VM Desktop Adapter"
PCIE1EMBEDDED.DeviceDesc       = "82562EH based Phoneline Desktop Adapter"

PCIE100EMBLOM.DeviceDesc     = "Intel(R) PRO/100 VE Network Connection"
PCIE100PLUSEMBLOM.DeviceDesc = "Intel(R) PRO/100 VM Network Connection"

PCIE100EMBLON.DeviceDesc     = "Intel(R) PRO/100 Network Connection"

PCIE100Sx.DeviceDesc       = "Intel(R) PRO/100 S Desktop Adapter"
PCIE100SxSVR.DeviceDesc    = "Intel(R) PRO/100 S Server Adapter"
PCIE100S0L.DeviceDesc      = "Intel(R) PRO/100 Network Connection"
PCIE100SxL.DeviceDesc      = "Intel(R) PRO/100 S Network Connection"
PCIE100DUALSx.DeviceDesc    = "Intel(R) PRO/100 S Dual Port Server Adapter"

PCIE100SCBLAN.DeviceDesc  = "Intel(R) PRO/100 S Mobile Adapter"
PCIE100SCBLANR.DeviceDesc = "Intel(R) PRO/100 SR Mobile Adapter"
PCIE100SCBCOMBO.DeviceDesc= "Intel(R) PRO/100 S Combo Mobile Adapter"
PCIE100SCBCOMBOR.DeviceDesc="Intel(R) PRO/100 SR Combo Mobile Adapter"

PCIE100BSPLUSD.DeviceDesc = "Intel(R) PRO/100 S+ Desktop Adapter"
PCIE100BSPLUSS.DeviceDesc = "Intel(R) PRO/100 S+ Server Adapter"

IBMFEK.DeviceDesc  = "Intel(R) PRO/100 VE Desktop Connection"
IBMFES.DeviceDesc  = "iSeries 2892 10/100 Ethernet Port"
DL_EMBLOM.DeviceDesc     = "Intel(R) PRO/100 VE Adapter"

SamsungHomePNA.DeviceDesc    = "Samsung HomePNA 1M CNR"

; NT service name
e100bnt.Service.DispName = "Intel(R) PRO Adapter Driver"

; CICH
PCIE100CICHEMBEDDED.DeviceDesc = "Intel(R) 82562 based Fast Ethernet Connection"
