# Manually Adding an Adapter

## Windows Me

1. From the Control Panel, double-click the Add New Hardware icon.

2. Select "Specify the location of the driver" and click Next.

3. Select "Display a list of all driver in a specific location..." and click Next.

4. Select "Network Adapter" form the list and click Next.

5. Insert the PRO/100 S adapter disk and click Have Disk.

6. Enter the appropriate drive for your disk media (A:, D:, etc.), and click OK.

7. Click OK at the Select Device dialog box.

8. The New Hardware Wizard displays the message that it has found the driver. Click Next.

9. Click Finish.

10. Restart your computer when prompted.

## Windows 98

1. From the Control Panel, double-click the System icon.

2. Click the Device Manager tab.

3. Double-click Other Devices or Network Adapters in the list area.

4. Double-click a PCI Ethernet Controller.

5. Click the Driver tab, then click Install Base Driver Only.

6. Click Next at the Update Device Driver Wizard.

7. Select "Display a list of all the drivers..." and click Next.

8. Insert the PRO/100 S adapter disk and click Have Disk.

9. Enter the appropriate drive for your disk media (A:, D:, etc.), and click OK.

10. Click OK at the Select Device dialog box.

11. The Update Wizard displays the message that it has found the driver. Click Next.

12. Click Finish.

13. Restart your computer when prompted.

## Windows 95

If the New Hardware Found dialog box does not appear at startup and you cannot connect to the network, check the Device Manager list to see if the new adapter is present. If it is not, follow these steps:

1. From the Control Panel, double-click the System icon.

2. Click the Device Manager tab.

3. Double-click Other Devices (question mark icon) in the list area.

4. Double-click a PCI Ethernet Controller.

5. Click the Driver tab, then click Install Base Driver Only.

6. Insert the Configuration and Drivers disk or CD in the appropriate drive, and at the Update Device Driver Wizard, select "No" and click Next.

7. Click Have Disk, insert the Configuration and Drivers disk in the appropriate drive, and click OK.

8. At the Select Device dialog box, click OK again.

9. Follow any prompts for Windows 95 installation disks and restart when prompted.

| NOTE: The Windows 95 system files are typically available on the Windows 95 CD in the win95 directory (D:\win95).

`Last modified on 9/18/03 1:08p Revision 1`