Installing Intel Network Drivers for Microsoft Windows NT

# Intel Network Drivers for Windows* 95

## Installing the Driver

Make sure that your Windows 95 installation CD or diskettes available; you are prompted for them when you install the new adapter.

1. After you put the adapter in the computer and connect the cable, start the computer. Windows detects the adapter as a PCI Ethernet device.

   | NOTE: If this dialog box does not appear and Windows 95 starts normally, add the adapter. See Manually Adding an Adapter.

2. Depending on your version of Windows 95, either the Update Device Driver Wizard or New Hardware Found window displays.

3. In either case, insert the Product CD in the drive. If an Autorun window displays, ignore it.
   If you have downloaded the driver from the Intel support website, transfer the files to the system.

4. Follow the instructions as you are prompted. When prompted for a path, type d:\ (for a CD-ROM drive) or the download location of the drivers and click OK.

5. When prompted, insert any Windows 95 installation disks.

6. When prompted, restart the computer.

7. Connect to your network by double-clicking the Network Neighborhood icon on the desktop.

For troubleshooting information, click Troubleshooting in the Table of Contents.

## Remove Existing Adapters

> 1. Double-click My Computer.

> 2. Double-click Control Panel.

> 3. Double-click System.

> 4. Click the Device Manager tab.

> 5. Double-click Network Adapters.

> 6. Select the adapter driver listed below the Network Adapters group and click Remove.

> 7. Click OK.

`Last modified on 2/06/04 10:00a Revision 1`