Virtual LAN under Windows

# Configuring VLANs in Microsoft* Windows*

In Microsoft Windows, you must use Intel® PROSet to set up and configure VLANs. For instructions, see the Intel PROSet topic in the Table of Contents (left pane).

In most environments, a maximum of 64 VLANs per adapter port or team are supported by Intel PROSet.

| CAUTION: Use Intel PROSet to add or remove a VLAN. Do not use the Network and Dial-up Connections dialog box to enable or disable VLANs. Otherwise, the VLAN driver may not be correctly enabled or disabled.

| NOTE: Itanium®-based systems support VLANs only in Windows Server 2003.

`Last modified on 9/08/05 6:58a Revision 5`