PCI Hot Plug Support for Windows* 2000 and XP

# PCI Hot Plug Support for Microsoft* Windows* Operating Systems

Intel® PRO/100, Intel® PRO/1000, and Intel® PRO/10GbE network adapters are enabled for use in selected servers equipped with PCI Hot Plug support and running Microsoft* Windows* operating systems.

PCI Hot Plug only works when you hot plug an identical Intel network adapter.

| NOTE: If you replace an adapter in a PCI Hot Plug slot, do not place the removed adapter back into the same network until the server has rebooted. The two adapters may have the same Virtual MAC address and create a conflict.

For more information on setting up and using PCI Hot Plug support in your server, see your hardware and/or Hot Plug support documentation for details.

`Last modified on 10/21/04 11:12a Revision 1`